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Assembly information

Information on engine configuration
· In this chapter, the engine is represented as "BASE CONFIGURATION" (refer to Par 1.3 - Par. 1.4 ).
· For the assembly of components not described in this chapter refer to Chap. 11 .
· The following are the components described in Chap. 11 .
 
11.1 Oil dipstick in cylinder head
 
11.2 Heater (replacement)
 
11.3 Idler gear (for 3 rd / 4 th PTO)
 
11.4 3 rd PTO (replacement)

11.5 4 th PTO (replacement)

11.6 3 rd + 4 th PTO (configurations)

11.7 Air filter (cartridge replacement)

11.8 Remote oil filter (disassembly and assembly)
 
11.9 Poly-V alternator belt (replacement and adjustment)
 
11.10 Tightening pulley and alternator for Poly-V belt
 



Assembly recommendations
· The information is laid out in sequence, the intervention methods have been selected, tested and approved by the manufacturer's technicians.
· This chapter describes the installation procedures for the assemblies and/ or individual components which have already been checked, overhauled or possibly replaced with original spare parts.
· Where necessary, reference to special tools during assembly operations is indicated and identified in Tab. 13.1 , hereinafter in Tab. 9.1 an example of a special tool ( ST_05 ).

 
  Tab. 9.1
	SPECIAL TOOLS

	"ST" Code

	Picture /draw
	DESCRIPTION
	PART NUMBER


	

ST_05
	[image: ]
	

Six nicks Key SN 8
	

ED0014603650-S


 
[image: ]     Important
 
 

· Before proceeding with operations, read  Par. 3.3.2 .
· To easily locate specific topics, the reader should refer to the analytical index or chapter index .
· The operator must check that:

· the components, the assemblies, the coupling surfaces of the parts are washed, clean and thoroughly dried;
· the coupling surfaces are undamaged;
· the equipment and tools are ready so that all work can be carried out correctly and safely;
· ensure that the working environment is safe.
· The operator must:

· carry out the procedures smoothly and safely. It is thus recommended to install the engine on a special rotating stand used when servicing engines to ensure the safety of the operator and the other individuals involved;
· tighten the assemblies and / or components in a criss-cross or alternating pattern, initially with a value lower than that preset, and then subsequently, with the tightening torque specified in the procedure;
· replace all seal gaskets after each assembly for all components on which they are provided.



Engine block assembly
	9.3.1 Crankshaft bushings
 
[image: ]   Important
 
 
· Execute the procedure in Par. 8.2.1 and 8.2.2 , before proceeding with assembly.
· The crankshaft half-bearings are made of special material. Therefore, they must be replaced every time they are assembled to prevent seizures.
1. Fit the new half-bearings B onto the crankcase upper half E adhering to the reference notches C .
 
[image: ]   Important
 



· After the half-bearings are fitted, check that the lubrication holes D correspond with the crankcase grooves E .
· The lower and upper half bearings CANNOT be singularly replaced, and both halves must be replaced together.


1. Fit the new half-bearings A onto the lower crankcase F using the reference notches G .
2. Lubricate the half-bearings A and B with oil.
	[image: ]
Fig 9.1[image: ]


Fig 9.2

	9.3.2 Tappets


1. Lubricate the tappets G with oil.
2. Insert the tappets G into the housings H of the upper crankcase.
	[image: ]
Fig 9.3

	9.3.3 Camshaft


1. 
Check that the bushing Q is correctly fitted.
2. Lubricate the pins L , the cams M of the camshaft N , all the housing P ( Par. 8.2.4 and Par. 8.2.6 ) and the bushing Q with oil.
3. Insert the camshaft N all the way into its housing P .
4. Fit the lock ring R on to the crankcase E to hold the position of the camshaft N .
5. Manually rotate the camshaft N ensuring that it is free.
	[image: ]
Fig 9.4

	9.3.4 Vent compartment closure lid


1. 
With the screws CF tighten the cover CG and the gasket CH  (tightening torque to 10 Nm ).
	[image: ]
Fig 9.5

	9.3.5 Crankshaft
 
[image: ]   Important
 
 
· Carry out the checks described in Par. 8.4.1 and Par. 8.4.2 .


1. Check that the crankshaft half-bearings are mounted correctly on the upper crankcase E .
2. Lubricate the main journal and crankpin J , with oil.
3. Insert the crankshaft W into its seat on the upper crankcase E .
4. Insert the 2 shoulder half-rings K , between the crankshaft W and the upper crankcase E ( AB detail).
	[image: ]
Fig 9.6

	9.3.6 Lower crankcase
 
[image: ]   Important
 
 
· Before proceeding to the assembly of the piston and connecting rod, carry out the checks described in Par. 8.5.1 .


1. Check that the crankshaft half-bearings are mounted correctly on the lower crankcase F ( AC detail).
2. Assemble the 2 shoulder half-rings AD onto the lower crankcase F applying two drops of oil to keep them in their seat.
3. Check that the coupling surfaces AE are free from dirt and grit.
	[image: ]
Fig 9.7

	1. Spread a bead of Loctite 5660 (rif. AL) of approx 1 mm thickness on the surface AM of the upper crankshaft half C  being careful not to block the oil feed grooves AG and the return oil sump AH .
2. Join the two crankshaft halves E and F observing the guide pins AN .
 
[image: ]   Important
 
 
· Failure to follow the bolting procedures compromises the functionality of the engine and can cause damage to people and property.
	[image: ]
Fig 9.8

	1. Tighten the fastening screws strictly following the sequence and the tightening torque indicated.

 

Tightening Screws Torx M12x1,25 (from the n° 1 to the n° 10 ):
CYCLE 1 - with a torque of 40 Nm ;
CYCLE 2 - with a torque of 70 Nm ;
CYCLE 3 - with a torque of 120 Nm .

 

Tightening Screws Torx M8 (from the n° 11 to the n° 27 ):
CYCLE 4 - with a torque of 20Nm ;
CYCLE 5 - with a torque of 35 Nm ;


1. Perform the operations described in  Par. 8.4.2 .
2. Check that crankshaft W rotates smoothly.




	[image: ]
Fig 9.9

	9.3.7 Piston rings


1. Perform the operations described in Par. 8.5.3 .
2. Put the scraper ring AP onto the piston AQ .
3. Put the 2° seal ring AR on the piston AQ .
4. Put the 1° seal ring AS onto the piston AQ .
	[image: ]
Fig 9.10

	1. Perform the operations described in Par. 8.5.4 .
2. Position the segment openings with a 120° angle between them ( Y ).


NOTE:  do not use the segment opening with the pin hole ( N )


1. Lubricate the piston skirt and piston rings with oil.
	[image: ]
Fig 9.11

	9.3.8 Piston

 
[image: ]   Important
 
 
· Before proceeding to the assembly of the piston and connecting rod, carry out the checks described in Par. 8.5.1 .
· Always replace the bearings CE after each assembly.
· Mate components respecting references at Par. 7.13.5.
1. Loosen the screws AU and remove the connecting rod cap AV .
2. Fit the new bearings CE .
3. Insert the connecting rod AZ into the piston AQ and align the seats BA .
4. Insert the gudgeon pin BB into the seat BA for the assembly of the connecting rod and piston unit.
5. Insert the lock rings BD inside the seat BE of the piston AQ to lock the gudgeon pin BB .
[image: ]
Fig 9.13
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Fig 9.12





	9.3.9  Piston and connecting rod assembly

 
[image: ]   Important
 
 
· Before assembling the piston and connecting rod assemblies, execute the controls described in Par. 8.5


1. Rotate the crankshaft W by moving the crankpin BG to a TDC position of the affected cylinder.
2. Lubricate the piston skirt and rings AQ .

 


	[image: ]
Fig 9.14

	1. Check that the half-bearing AS is mounted correctly and lubricate it thoroughly.

 
 
[image: ] Important
 
 
· Make sure you are at the stage described in Point 1 .
· The piston AQ must be mounted with the arrow BN (stamped on the piston crown) facing the timing system side.


1. Using the piston ring compression pliers, insert the piston inside the cylinder BQ by around 10mm (height BM ).
	[image: ]
Fig 9.15

	1. Rotate the piston AQ by 10° counter-clockwise with respect to its correct assembly position ( Fig. 9.16 - height BP ).

 
	[image: ]
Fig 9.16

	NOTE : Doing this prevents the impact between the connecting rod AZ and the sprayer V .


	[image: ]
Fig 9.17

	[image: ]     Important
 



· Leave the ring compressor assembled on the piston

 
 
1. Push piston AQ downwards without introducing the segments in the cylinder, rotate piston AQ by 10° in a clockwise direction (value  BR – correct assembly position).


[image: ]
Fig 9.18



	1. Push the piston AQ downwards by centering the crankpin BG with the connecting rod AZ .
2. Turn the crankcase on support to assemble the con rod capp on cylinder 1 and 4 .
3. Check that the half-bearing AS is mounted correctly on the connecting rod cap AV .


	[image: ]
Fig 9.19

	[image: ]     Important
 



· Check that the break levels of connecting rod cap AV coincide perfectly onto connecting rod AZ before screwing on and tightening capscrews AU .


1. Couple the connecting rod cap AV to the connecting rod AZ using the marks made at disassembly ( Par. 7.15.2 e 7.15.5 ).
2. Screw in the screws AU .
3. Repeat the operations from 1 to 10 for each cylinder.

 
 
[image: ]     Important
 



· Failure to adhere to the assembly procedures may compromise the functionality of the engine, and also cause damage to persons and property.

 


1. Tighten the screws AU , alternately, strictly following the tightening torques indicated.

 
Tightening sequence of screws Torx M10x1:
 
1° CYCLE - with a torque of 40 Nm ;
2° CYCLE - with a torque of 85 Nm ;

 
2. Check that the connecting rods have axial play and the crankshaft W rotates smoothly.

 
NOTE : After the check carried out at point 14, position the shaft W with the first cylinder to TDC.


	[image: ]
Fig 9.20





	9.3.10 Crankshaft gasket flange
 
 
 
[image: ]   Important
 
 
· Check that the contact surface between the flange and the crankcase is free of grit and dirt.
· Always replace the gasket BS after each assembly.

 
1. Check that there are bushings BT on the crankcase E .
2. Lubricate the oil seal lip BU .
3. Position the gasket BS and flange BV on the crankcase E in correspondence with the bushings BT .
4. Put Loctite 243 on the 2 screws BW matching the bushings BT .
5. Screw the fastening screws all the way in BW without tightening them.
6. Tighten all the screws BW strictly following the tightening sequence indicated (tightening torque to 10 Nm ).
	[image: ]
Fig 9.21 a[image: ]


Fig 9.21 b


	9.3.11 Cover 3 rd PTO
 
[image: ]   Important
 
 
· Replace capscrews CA with each assembly or alternatively apply Loctite 2701 on the thread.


1. Secure the cover CB with the screws CA and CC inserting the gasket CD (tightening torque 25 Nm ).
	[image: ]
Fig 9.22


 



Oil sump unit assembly
	9.4.1 Oil fume pipes


1. 
Apply Loctite 648 on the pipe threads A .
2. Screw and tighten the pipes A (tightening torque of  15 Nm ).
	[image: ]
Fig 9.23

	9.4.2  Oil suction pipe
 
[image: ]   Important
 
 
· It is mandatory to replace the gasket B after each assembly.
· Always replace capscrews D with new ones or alternatively apply Loctite 2701 .

 
1. Insert the new gasket B in the seat of the oil suction hose flange D .
2. Secure the hose C on the crankcase E with the screws D (tightening torque 10 Nm ).
	[image: ]
Fig 9.24

	9.4.3 Oil Sump


1. Ensure that the contact surfaces F of the oil sump G and the crankcase E are completely clean.
2. Apply a bead of approx. 2.5 mm of sealant (Loctite 5660) on the surface F of the oil sump G .
3. Note : alternatively apply Loctite 5699 .
	[image: ]
Fig 9.25

	[image: ]     Important
 
 
· Tighten the screws L , strictly following the sequence and tightening torque indicated.

 
1. Tighten the screws L following the sequence indicated (tightening torque 25 Nm ).
2. Remove the two studs ST_18 with the appropriate screws (tightening torque 25 Nm)
3. After tightening all of the screws, loosen screw n°1 and retighten it to the torque value specified in step 4 .
4. Check that the oil drain plugs M are tight (tightening torque 35 Nm ).
	[image: ]
Fig 9.26


 



Flange unit assembly
	9.5.1 Bell housing

 
[image: ]   Danger
 
 
· Bell A is very heavy; pay special attention during assembly operations to avoid dropping and causing serious risks to the operator.


1. Install the bell housing A in accordance with the reference pins B on the base C .
	[image: ]
Fig 9.27

	[image: ]   Important
 
 
· Failure to adhere to the assembly procedures may compromise the functionality of the engine, and also cause damage to persons and property.


1. Tighten the fastening screws D strictly following the tightening sequence indicated (tightening torque 50 Nm ).
	[image: ]
Fig 9.28

	9.5.2 Flywheel
 
[image: ]   Danger
 
 
· Flywheel F is very heavy; pay special attention during assembly operations to avoid dropping and causing serious risks to the operator.


1. Screw the special tool ST_09 on the crankshaft E instead of the screws G positioned higherup ( Fig.  9.29 ).
2. Insert the flywheel F on the crankshaft E using the tool as a guide ST_09 and manually tighten all the screws G (the last screw is fitted in the place of the tool ST_09 ).
3. Mount the tool ST_34 in the seat of the starter motor H and fit it with the two starter motor fixing screws.
4. Tighten the screws G (tightening torque at 140 Nm ).
	[image: ]
Fig 9.29


 



Timing system gear assembly and injection pump
	9.6.1 Timing system gear assembly


1. Check that the key A is correctly fitted on the camshaft B .
2. Position the gear C on the camshaft B adhering to the key reference A .
3. Screw capscrew D until the end.
4. Tighten the middle gear pin H , in the housing J of the crankcase, with the screws K (tightening torque 25 Nm ).


	[image: ]
Fig 9.30

	[image: ]   Important
 
 
· The fitting of the middle gear pin H has only one position, the 4 screw holes K are asymmetric.
· Always replace the gasket L at each assembly.




1. Insert the shoulder ring M .
2. Check the integrity of the bushing N into the middle gear P , and ensure that it is free from impurities.
3. Thoroughly lubricate the pin H and the bushing N .
4. Position the gear P on the pin H observing all the marks W of the gears C and S (Fig. 9.30) .
	[image: ]
Fig 9.31

	[image: ]   Important
 
 
· Failure to comply with the marks W on the gears C, P and S , causes engine malfunction and serious damage.
	[image: ]
Fig 9.32

	1. Insert the shoulder ring Q and the lock ring R.
2. Tighten the screw D ( Fig. 9.30 - tightening torque at 100 Nm ).
	[image: ]
Fig 9.33

	9.6.2 Injection pump



 
[image: ]   Important
 
 
· Always change screws T with new ones or alternatively apply Loctite 270 (Fig. 9.34) to the threads.




1. Perform the operations described in the warning in Par. 6.1.5 .
2. Place a dial gauge to detect the TDC on piston N° 1 , then bring the indicator of the dial gauge to 0 .
NOTE : During the detection phase of the TDC, check that cylinder N° 1 is in compression phase (align the notches W as in Fig. 9.33 ).


	[image: ]
Fig 9.34
 
 
 

	1. By means of the identified pump code, refer to Tab. 6.1 to know the advance degrees and the corresponding value to lower the piston.
2. Mount tool ST_34 in the seat of starter motor H (Fig. 9.29) and fix it with two motor fixing screws.
3. Having identified the value to lower the piston, rotate the crankshaft anti-clockwise by going beyond the value described in Tab. 6.1 , once again, rotate the crankshaft clockwise stopping at the correct advance value by using tool ST_03 - ST_34 .
4. Lock the ST_34 , ensure that the crankshaft does not rotate, which would alter the correct advance value.
If this happens, repeat the instructions described in points 4, 5 and 6.
	[image: ]
Fig 9.35

	1. Fix pump Z into housing V by means of screws T ( Fig. 9.34 - tightening torque at 25 Nm ).
2. Position the gear AC onto shaft AB of the pump.


NOTE: You are not required to respect the reference Q gear AE ( Fig. 9.36 ).


1. Insert washer U and tighten nut AD (tightening torque at 70 Nm ).
  
[image: ]   Important
 
 
· In the event of assembling screw X1 (tightening torque at 10 Nm ).
· In the event of assembling screws X2 and X3 (tightening torque at 2 5 Nm ).
	[image: ]
Fig 9.36


[image: ]
Fig 9.37


 



Cylinder head unit assembly
	9.7.1 Valve stem gasket

 
[image: ]   Important
 
 
· Carry out the checks described in Par. 8.6.4 before proceeding with the following operations.
· Always replace gasket A with every assembly
· Lubricate the gaskets A on the inside.
1. Fit the oil seals A on the valve guides B using the tool ST_08 .
	[image: ]
Fig 9.38

	9.7.2 Injector sleeves  ( [image: ] )


1. Insert the seals C in the seats of the sleeve D .
2. Insert the seal E with the convex side facing upward at the base of the sleeve D .
3. Lubricate the gaskets C .
4. Insert and carefully screw the sleeve D into the seat of the head F .

 
NOTE: The sleeve D must not protrude above the surface of the head BF .

 
5. Clamp the sleeve D (tightening torque at 30 Nm ).
	[image: ]
Fig 9.39

	9.7.3 Injectors projection


1. Insert the injector G inside the sleeve H .
2. Mount the injector fixing bracket M and secure it with the screw N , without performing the calibration.
3. Check protrusion of injectors by means of the tool ST_03 (Fig. 9.44) , check the projection of the injector, which must range between 1.68 ÷ 2.42 mm.

 
NOTE : if the value detected does not correspond, replace gasket Q with a different thickness.
	[image: ]
Fig 9.40[image: ]


Fig 9.41

	9.7.4 Valves


1. Pre-lubricate and insert the valves X into the head F taking care to fit them in the original positions as per the reference marks made in Par. 7.11.3.1 .
2. Position the spring Y on the seat of the head F .
3. Position the disk S on the spring Y centering the valve X .




































1. Mount the tool ST_07 on the head F fixing it on one of the holes for securing the rocker arm cover.

 
NOTE: Change the fixing hole according to the position of the valves to be fitted.

 
2. Position the tool ST_07 on the valve as shown in the figure.












1. Push the lever of the tool ST_07 downwards, in order to lower the valve disks S in the direction of the arrow AK , and insert the valve cotters AJ inside the disk S .
2. Check that the valve cotters AJ are properly mounted on the valve seats X and release the tool ST_07 .

 
NOTE: repeat all the steps for the relevant valves and remove the tool ST_07 .
	[image: ]
Fig 9.42

	
	[image: ]
Fig 9.43

	
	[image: ]
Fig 9.44

	9.7.5 Cylinder head


1. 
Fix the eyebolts AW with the screws AX onto the head F (tightening torque of 25 Nm ).
2. Position the piston P at the TDC.
3. Position the tool ST_03 on the crankcase surface of the head and measure the piston protrusion P from head level K in 4 diametrically opposed points R. Repeat the operation for all pistons P and take note of the highest average value, determining valu e S (Tab. 9.2) .

 
Tab. 9.2

	S (mm)
	Hole number

	

0.030 - 0.126
	1 [image: ]

	

0.127 - 0.250
	2 [image: ]

	

0.251 - 0.375
	3 [image: ]



4. Based on the value detected at point 3 , select the relevant gasket T as shown in the Tab. 9.2 (Fig. 9.47 detail U ).
5. Check that the crankcase surface K and the gasket T are completely free of dirt and grit.

 
 
[image: ]   Important
 
 
· The head gasket must be replaced for each assembly.


1. Position the gasket T on the surface K with reference to the centering bushings J .
	[image: ]
Fig 9.45[image: ]


Fig 9.46[image: ]


Fig 9.47

	1. Check that the surface head W is free from impurities.
2. Position the head F on the crankcase Z with reference to the centering bushings J .

 
 
[image: ]   Important
 
 
· The fastening bolts V must be replaced every time they are assembled.
· Failure to adhere to the bolt fixing procedures may compromise the functionality of the engine, and also may cause damage to persons and property.
· Tighten capscrews V observing the cycles, tightening, and subsequent rotation as indicated in Tab. 9.3 .




1. Secure the head F by tightening the screws V strictly following the sequence indicated in the Fig. 9.50 and the tightening torque indicated in the Tab. 9.3 .
	[image: ]
Fig 9.48

	Tab. 9.3

	CYCLE
	TORQUE

	1
	40 Nm

	2
	70 Nm

	3
	100 Nm

	4
	90°

	5
	90°

	6
	90°



	[image: ]
Fig 9.50

	9.7.6 Rods and valve bridges


1. Insert the rocker control rods AA into the niches of the head F .
 
[image: ]   Important
 
 
· Properly centre the rods AA into the spherical housing of the camshaft tappets AB .
1. Mount the valve bridge AC on to the pairs of discharge and suction valves.
	[image: ]
Fig 9.51

	
	[image: ]
Fig 9.52

	9.7.7 Rocker arms

 
[image: ]   Important
 
 
· To correctly position the rocker arms, turn the rocker arm pin AH with the lower height AL towards the timing system side as in Fig.9.54 .
· The discharge rocker arm AT is shorter than the suction arm AR .

 
1. Fit the lock ring AM into the seat AN of the rocker arm pin AH .
2. Position the pin AH with the screw support surface AP facing upwards and insert the 2 shoulder rings AQ .
3. Insert in sequence the suction rocker arm AR , the holder AS and the discharge rocker arm AT in the pin AH .
4. Insert the spring AU in the pin AH .
5. Repeat points 3, 4 for all the rocker arms.
NOTE: The holder AV must be fitted with the last pair of rocker arms towards the flywheel.
6. Insert 2 shoulder rings AQ and the lock ring AN to lock all the components inserted in the pin AH .
NOTE : The spring AU ensures that the supports AS and AV are kept in place.
	[image: ]
Fig 9.54[image: ]


Fig 9.55

	9.7.8 Rocker arm pin assembly

 
[image: ]   Important
 
 
· Position the rocker arm pin assembly BB on a level to align all the support surfaces.
· Check that the pistons are positioned half way between the TDC and BDC. Rotate the crankshaft 90° counterclockwise with regard to the 1st cylinder TDC, positioning the crankshaft pin BP as shown in Fig 9.58a . If the crankshaft pulley and the timing gear cover have not been removed, rotate the
crankshaft positioning the reference BQ located on the target wheel in correspondence of the speed sensor, as shown in Fig. 9.58b .

 
1. Position the rocker arm pin assembly BB on the head F , respecting the plug BC on the head using the holder indicated AV .
2. Check the correct positioning of all the rocker arms and the u-bolt control valves (detail BD ). House the tappet in the seat of the rocker arms control rod.
3. Secure the rocker arm pin BB tightening the screws BE (tightening torque to 25 Nm ). Adhere to the screw tightening sequence BE as shown in Fig. 9.60 .
	[image: ]
Fig 9.56[image: ]


Fig 9.57

	[image: ]
Fig 9.58a
	[image: ]
Fig 9.58b


 



Fuel system assembly
	[image: ]   Important
 
 
· Replace the high pressure pipes after two disassemblies.
· Remove the protective caps from all the components of the fuel circuit just before assembly (Par. 2.9.7).
· When repaired, RSN-A injectors must be certified by a Stanadyne centre to check their correct operation - check the type of engine mounted injectors on the spare parts list ( RSN-A is specified in the description).
	[image: ]
Fig 9.59

	
9.8.1 Injector

 
1. Lubricate the gaskets U, T, S , and fit them on the injector Z.
	[image: ]
Fig 9.60

	  2 .  Fit the injector Z in the sleeve V .
	[image: ]
Fig 9.61

	
1. Assemble parts P, Q, R .
2. Fit the parts so assembled on the injector Z .
	[image: ]
Fig 9.62

	5. Insert tool ST_51 on the injectors junctions Z (detail X1 ).
6. Tighten the screw P (tightening torque to 20 Nm )
	[image: ]
Fig 9.63

	
 
9.8.2 Fuel injector ricicle pipe
 
1. Position the tube N on the injectors Z , and tighten screws M (coppia di serraggio a 14 Nm ) and insert the gasket T .
	[image: ]
Fig 9.64

	9.8.3 Rocker arm cover


[image: ]
 Important

· Always replace the gaskets AK after each disassembly ( ST_36 ).
1. Position tool ST_17 onto the head in correspondence with the two fastening holes 5 and 6 ( Fig. 9.67) .
2. Position the gasket AM on the head AL using tool ST_17 as a guide.
3. Fit the rocker arm cap C on the head AL via the screws L observing the clamping sequence illustrated in Fig. 9.67.
4. With vaseline lubricate the gaskets AK.
	  [image: ]
Fig 9.65




[image: ]
Fig. 9.67

	9.8.4 Installation of the fuel injector pipes (injection pump/injectors)

 
[image: ]   Important
 



· Replace the high pressure pipes after two disassemblies.
 
 
1. Position pipes D on the injectors and on the injector pump and tighten the nuts E and F manually, without clamping them.
2. Clamp the nuts E and F (tightening torque at 25 Nm ).
3. Mount the retainers C of the hoses D.
	[image: ]
Fig 9.68

	


9.8.5 Fuel filter


1. Secure the fuel filter holder J with the screws K on the crankcase W (tightening torque of 25 Nm ).

 
NOTE: For the assembly of the fuel cartridge, refer to operation 2 of Par. 6.7.2 .


	  [image: ]
Fig 9.69


 



Intake manifold assembly
	[image: ]   Important
 
 
· Check that the contact surfaces between the collector C and the head D are free from impurities.
1. Insert ST_18 special tool into market point.
2. Mount the gasket A on the head D .
3. Mount the manifold C on the head D .
4. Fit the manifold C using the screws B (tightening torque of 25 Nm ).
	[image: ]
Fig 9.70


 



Exhaust manifold assembly
	[image: ]     Important
 
 
· Replace the self-locking nuts B and the metal gaskets D between the manifold and the cylinder head every time they are assembly.
· In the event of mounting the studs C , fix ( 25 Nm tightening torque) with Loctite 2701 on the thread.

 


1. Check that the contact surfaces F are free from impurities.
2. Insert the gaskets D and E on the studs C .
3. Position the manifold A on the studs C .
4. Fix the manifold A on the cylinder head by tightening the self-locking nuts B (tightening torque of 25 Nm ).
	[image: ]
Fig 9.71





Lubrication circuit assembly
	9. 11 .1 Assembly oil mist separator unit


1. Follow operations 1, 3, 4, 6, 7 and 8 of Par. 6.8.2.

	9. 11 .2 Oil Cooler and oil filter Unit Assembly
 
1. Follow operations of Par. 6.6.2 - 6.6.3 .

	9. 11 .3 Oil pump

NOTE: Carry out the checks described in Par. 8.7 before proceeding with the following operations.
 
1. Check that all contact surfaces between AL, AH, AF, AG and AN are free of impurities – scratches - dents.
2. When assembling, do not use any type of gasket between  AG and AN.
3. Thoroughly lubricate the seat of the rotors AF on the oil pump crankcase AG and the two rotors AH and AL .
4. Insert, inside the seat AF , the 2 rotors (in sequence) AH and AL , respecting the reference BP as the picture. (or refer to Par. 2.10.2 ) .
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Fig 9.73

	1. Check that the 2 pins AM are inserted properly in the crankcase timing system AN .
2. Position the oil pump assembly AG using the pin marks AM .
3. Fasten the oil pump cover AG with the screws AH (tightening torque 10 Nm ).
	[image: ]
Fig 9.74

	9. 11 .4 Timing system crankcase
 
[image: ]   Important
 
 
· Always replace the oil seal J after each assembly ( ST_14 ).
· Always replace the gasket P after each assembly.
· To prepare the surface of the K plane for the new application of the sealant, it must be cleaned through the use of:
- initially Loctite SF 7200
- subsequently Loctite SF 7063
Avoid any contact with the K plane and be careful not to compromise the cleaning performed.
1. 

Distribute a bead of Loctite 5188 , of about 1mm thickness, on the surfaces K of the crankcase C .
2. Make sure that the key M ( Fig. 9.76 ) is inserted properly on the crankshaft and that it is facing upwards.
3. Lubricate and insert the gasket P in the seat of oil pump Q .
	[image: ]
Fig 9.75



	 

1. Tighten the tool ST_10 on the crankshaft.
2. Check that the 2 pins N are properly inserted in the timing system crankcase C .
3. Lubricate the gasket J with oil and position the crankcase C on the crankcase E , using the pins N , inserting the oil pump Q on the crankshaft. 

	[image: ]
Fig 9.76

	1. Fasten the screws R (tightening torque of 25 Nm ).
	[image: ]
Fig 9.77

	9. 11 .5 Crankcase oil filler flange Timing System
 
[image: ]   Important
 
 
· Always replace the gasket BA after each assembly.


1. Position the gasket BA in the seat on the flange BB .
2. Clamp the flange BB on the crankcase BC with the screws BD (tightening torque of 10 Nm - ST_06 ).
	[image: ]
Fig 9.78

	9. 11 .6 Oil pressure relief valve


1. Lubricate the piston BE and fully insert it in the seat BF .
2. Insert the spring BG in the piston.

 
 
[image: ]   Important
 
 
· Always replace the gasket BH after each assembly.


1. Mount the gasket BH on cap BL .
2. Tighten the cap BL on the crankcase BC (tightening torque of 50 Nm ).
	[image: ]
Fig 9.79



 



Crankshaft pulley assembly
	1. Check that the pin U is mounted properly on the crankshaft V .
2. Position the pulley T on the crankshaft V using the pin mark U .
3. Apply Molyslip grease on the screw thread Z .
4. Clamp the pulley T with the screw Z (tightening torque of 360 Nm ) and remove special tool ST_34 ( Fig. 9.29)
	[image: ]
Fig 9.80


 



Turbocharger Assembly
	[image: ]   Important
 
 
· Before proceeding, perform the operation described in Par. 2.18 .
· Ensure that tube B is not clogged.
1. Fasten the connecting sleeve A to the pipe B with the clamp C onto the flange fitting D .

 
 
[image: ]   Important
 
 
· Always replace the gasket F after each assembly.




1. Lubricate and insert the gasket F into the seat of the pipe G .

 
 
[image: ]   Important
 
 
· Remove the plastic or foam caps from the turbo compressor before assembling.
· Replace nuts M with each assembly.


1. Check that the contact surfaces E are free from impurities deformations or cracks, otherwise replace exhaust manifold L .
2. Position the turbo-compressor H on the bolts on the manifold L .
3. Fasten the turbo-compressor H with the nuts M (tightening torque of 25 Nm ).
4. Insert the sleeve T on the turbo-compressor H and secure it with the clamp U .
5. Fasten the pipe G with the screws N to the turbo-compressor H .
 
[image: ]   Important
 
 
·  Always replace the gasket P after each assembly.
· Before assembly of the tube Q , perform the operation described in Par. 2.18.2 - point 2 .
· Ensure that tube Q is not clogged.


1. Insert the gaskets P between:
- Q and R ;
- Q and S ;
- Q and H .
Fasten the fuel outlet pipe Q with the fittings R on the turbo-compressor H and on the crankcase S (tightening torque of 15 Nm ).

 
2. Follow operations 4 and 5 of Par. 6.1.9 .
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Fig 9.81[image: ]


Fig 9.82[image: ]


Fig 9.83


 



Coolant circuit assembly
	9.14.1 Thermostatic valve
 
[image: ]     Important
 
 
· Always replace the gasket A after each assembly.

 
1. Check the condition of the seal gasket A and fit it on the thermostatic valve B .
2. Position the thermostatic valve B in the seat on the head C (detail D ).
3. Secure the cover E with the screws F on the head C (tightening torque of 10 Nm ).
	[image: ]
Fig 9.84

	9.14.2 Coolant pump

 
[image: ]   Important
 
 
· Always replace the gasket L every time it is assembled.

 
1. Fit the pump G with the screws H interposing the gasket L (tightening torque of 25 Nm ).
	[image: ]
Fig 9.85

	9.14.3 Oil Cooler hoses


1. 
Fit hose Q1 onto coolant pump G and Oil Cooler M .
2. Fit hose Q2 onto crankcase R and Oil Cooler M .
3. Secure the sleeve Q on Oil Cooler M and to the pump G with the clamps K .
4. Fasten the clamp Y with the screw S (tightening torque of 22 Nm - ST_05 ).




[image: ]
Fig 9.86


 



Electric component assembly
	9.15.1 Sensors and switches

	9.15.1.1 Coolant temperature sensor


1. Secure the sensor D onto the head E (tightening torque of 20 Nm ).
	[image: ]
Fig 9.87

	9.15.1.2 Oil pressure switch


1. 
Clamp the oil pressure switch F on the crankcase G (tightening torque at 35 Nm ).
	[image: ]
Fig 9.88

	9.15.1.3 Fuel filter water detection sensor


1. Lubricate and insert the gasket AA on the fitting AB .
2. Fix the sensor AB onto the cartridge AC (tightening torque of 5 Nm ).

 
	[image: ]
Fig 9.89



	9.15.2 Alternator


1. Mount the bracket M  on the head N using the screw H and relative washer, without clamping it.
2. Fit the alternator with the screw A with the relative washer and spacer B .
3. Mount the alternator C on the crankcase Q  tightening the nut R  up to the stop without clamping it.
4. Mount the screw L and relative washer on the alternator C , without clamping it.
5. Clamp screw H (tightening torque of 25 Nm ).


	[image: ]
Fig 9.90



	[image: ] Important
· The belt S must always be replaced every time it is assembled, even if it has not reached the scheduled hours for replacement.






1. Insert the belt E on the pulleys T .
2. Push the alternator C in the direction of the arrow J .
3. While tensioning the alternator C , first clamp screw A (tightening torque at 25 Nm ) and then screw  D  (tightening torque at 69 Nm [thread M10] - 40 Nm [thread M8] ).
4. Check the tension of the belt S  with the instrument ( DENSO BTG-2 ), positioning it in point P (the tension must be between 200 and 230 N ).
5. If the tension values do not correspond, tighten screws A and D, then repeat operations 7 , 8 , 9 and 10 .
	[image: ]
Fig 9.91



	9.15.3 Starter Motor
 
[image: ]   Important
 
 
· Remove the tool if still there ST_34 .


1.  Fit the starter Q with the screws R on to the flange bell S (tightening torque of 45 Nm ).
	[image: ]
Fig 9.92


 



Tightening torques and the use of sealants
Tab. 9.4 - * Alternatively to the capscrew replacements, with "Dri-loc"
	BASE CONFIGURATION

	SHORT BLOCK

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Breather room closing cover fastening capscrew (EXHAUST SIDE)
	M6x1
	10
	 

	Lower crankcase fastening capscrew

	M12x1.25
	3 Torque cycles
	 

	1st Cycle
	 
	40
	 

	2nd Cycle
	 
	70
	 

	3rd Cycle
	 
	120
	 

	Lower crankcase fastening capscrew

	M8x1.25
	2 Torque cycles
	 

	1st Cycle
	 
	20
	 

	2nd Cycle
	 
	35
	 

	Connecting rod screw
	M8x1
	2 Torque cycles
	 

	1st Cycle
	 
	40
	 

	2nd Cycle
	 
	85
	 

	Crankshaft gasket flange fastening capscrew
	M6x1
	10
	 

	Closing cover fastening capscrew 3 rd PTO
	M8x1.25
	25
	Loctite 2701*

	Idle gear lubr. hole cap closure
	M14x1.5
	30
	Loctite 2701*

	Coolant drain hole closing cap
	M16x1.5
	50
	 

	OIL SUMP ASSEMBLY

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Oil fumes tube
	M12x1,5
	15
	Loctite 648

	Oil suction hose fastening capscrew
	M6x1
	10
	Loctite 2701*

	Oil sump fastening capscrew
	M8x1.25
	25
	 

	Oil drain cap
	M18x1.5
	35
	 

	FLANGE ASSEMBLY (1st PTO)

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Flange bell fastening capscrew
	M10x1,5
	50
	 

	Flywheel fastening capscrew
	M12x1,25
	140
	 

	GEAR DISTRIBUTION

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Intermediate gear gudgeon fastening screw
	M8x1.25
	25
	 

	Camshaft gear control fastening capscrew
	M10x1
	100
	 

	Fastening nut on fuel injection pump gear
	M14x1.5
	65
	 

	ENGINE CYLINDER HEAD ASSEMBLY

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Air bleeding cap
	M6x1
	8
	 

	Lifting brace fastening capscrew
	M8x1.25
	25
	 

	Injector manifold
	M12x1
	30
	 

	Cylinder head fastening capscrew

	M12x1.25
	6 Torque cycles
	 

	1st Cycle
	 
	40
	 

	2nd Cycle
	 
	70
	 

	3rd Cycle
	 
	100
	 

	4th Cycle
	 
	90°
	 

	5th Cycle
	 
	90°
	 

	6th Cycle
	 
	90°
	 

	Rocker arm gudgeon fastening capscrew
	M8x1,25
	25
	 

	Rocker arm cover fastening capscrew
	M6x1
	10
	 

	INJECTION SYSTEM

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Injector brace fastening capscrew
	M8x1.25
	20
	 

	Waste line fastening drilled capscrew/nipple on Cyl. head
	M6x1
	14
	 

	Waste line fastening drilled capscrew on injectors
	M10x1
	15
	 

	Injector side injection tube nuts
	M12x1.5
	25
	 

	Injection pump side injection tubes nuts
	M12x1.5
	25
	 

	Injection pump fastening capscrew
	M8x1.25
	25
	Loctite 2701*

	Fuel injection pump locking screw
	...
	 
	 

	Fuel delivery fastening drilled capscrew (on injection pump)
	M10x1
	25
	 

	Waste line fastening drilled capscrew (on injection pump)
	M10x1
	25
	 

	Bleeding screw injection pump (on waste line fastening drilled capscrew)
	M6x1
	22
	 

	Fuel filter fastening capscrew
	M8x1.25
	22
	 

	INTAKE MANIFOLD

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Fastening screw intake manifold
	M8x1.25
	25
	 

	Intake flange fastening capscrew
	M8x1.25
	25
	 

	EXHAUST MANIFOLD

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Exhaust manifold fixing stud
	M8x1.25
	25
	 

	Exhaust manifold fixing nut
	M8x1.25
	25
	 

	Exhaust flange/muffler fixing nut
	M8x1.25
	25
	 

	LUBRICATION CIRCUIT

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Oil filter fastening union
	M20x1.5
	15
	Loctite 2701*

	Oil filter
	M20x1.5
	15
	 

	Oil pump carter fastening capscrew
	TG6
	10
	 

	Carter distribution fastening capscrew
	M8x1.25
	25
	 

	Fastening capscrew for plug on timing system cover
	TG6
	10
	 

	Side oil load flange fastening capscrew (onto carter distribution)
	TG6
	10
	 

	Pressure relief valve cap
	M16x1.5
	50
	 

	Breather system cover fastening capscrew (on rocker arms cover)
	M8x1.25
	25
	 

	CRANKSHAFT PULLEY

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Crankshaft pulley fastening screw
	M16x1.5
	360
	Molyslip

	COOLANT CIRCUIT


	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Thermostatic valve cover fastening capscrew
	M6x1
	10
	 

	Coolant pump fastening capscrew
	M8x1.25
	25
	 

	ELECTRICAL COMPONENTS

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Coolant temperature sensor
	M12x1.5
	20 max.
	 

	Oil pressure switch
	M12x1.5
	35
	 

	Sensor for water presence in fuel
	 
	5
	 

	Alternator bracket fastening capscrew
	M8x1.25
	25
	 

	Alternator fastening capscrew
	M8x1.25
	40
	 

	Alternator fastening capscrew
	M10x1.5
	69
	 

	Starter motor fastening capscrew
	M10x1.5
	45
	 

	Supply cable fastening nut (starter motor)
	M8x1.25
	10
	 

	CONTROLS

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Accelerator bracket fastening capscrew
	M6x1
	10
	 


* Alternatively to the capscrew replacements, with "Dri-loc"
 
 
	OPTIONAL COMPONENTS (CHAP. 11)

	OIL DIPSTICK ON CYLINDER HEAD

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Oil dipstick tube fastening capscrew
	M6x1
	10
	 

	HEATER


	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Flange intake with heater fastening capscrew
	M8x1.25
	22
	 

	ALTERNATOR WITH POLY-V BELT

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Pulley fastening capscrew
	M10x1.5
	48
	 

	Pulley positioning blocking nut capscrew
	M10x1.5
	45
	 

	Alternator brace fastening capscrew
	M8x1.25
	25
	 

	Alternator fastening capscrew (upper)
	M8x1.25
	25
	 

	Alternator fastening capscrew (lower)
	M8x1.25
	40
	 

	Pulley sliding plate fastening capscrew
	M8x1.25
	25
	 

	IDLE GEAR (FOR 3TH /4TH PTO)

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Gear drilled fastening capscrew
	M14x1.5
	Consultare il Par. >>
	Molyslip

	3 TH PTO

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Pump support fastening capscrew
	M8x1.25
	25
	Loctite 2701*

	Pump fastening capscrew
	M8x1.25
	25
	 

	4 TH PTO

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Grooved crankshaft support fastening capscrew
	M8x1.25
	25
	Loctite 2701*

	Cover fastening capscrew (3 rd PTO side)
	M8x1.25
	25
	 

	Sump support fastening capscrew
	TG6
	10
	 

	Pump fastening capscrew
	M8x1.25
	25
	 

	BALANCE DEVICE (4 CYLINDERS)

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Housing closing panel fastening capscrew
	M6x1
	8
	 

	Shafts support fastening capscrew
	M10x1.5
	50
	 

	REMOTE OIL FILTER

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Head fastening and Oil Cooler union on crankcase
	M20x1.5
	25
	Loctite 2701*

	Crankcase head nipple and oil filter support
	M14x1.5
	40
	 

	Tube union on crankcase head
	G3/8
	30
	 

	Tube union on filter support
	G3/8
	35
	 

	Oil filter
	M20x1.5
	20
	 

	Filter support head air bleeding cap
	M8x1.25
	25
	 

	INTAKE CIRCUIT

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Air filter support plate fastening capscrew (on flange bell)
	M8x1.25
	25
	 

	Air filter support fastening capscrew
	M8x1.25
	25
	 

	EXHAUST CIRCUIT

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Muffler brace support fastening capscrew
	M8x1.25
	25
	 

	Muffler fastening capscrew on muffler
	M8x1.25
	25
	 

	Muffler fastening nut
	M8x1.25
	25
	 

	COOLING CIRCUIT

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Blower fastening capscrew
	M6x1
	10
	 

	Radiator support fastening capscrew
	M16x1.5
	150
	 

	Shroud radiator fastening capscrew
	M6x1
	10
	 

	Radiator lower brace fastening capscrew
	M8x1.25
	25
	 

	Radiator on anti-vibrating
	M8x1.25
	25
	 

	Anti-vibrating radiator fastening nut (on lower brace)
	M8x1.25
	25
	 

	Anti-vibrating and brace fastening capscrew (upper)
	M6x1
	10
	 

	Upper brace fastening capscrew (on engine cylinder head)
	M8x1.25
	25
	 

	Side bulkheads fastening capscrew
	M6x1
	10
	 

	ENGINE SUPPORT

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Side feet fastening capscrew (on flange bell or crankcase)
	M12x1.75
	50
	 

	Rear feet fastening capscrew
	M16x1.5
	200
	 

	OIL SUMP WITH SUPPORTING STRUCTURE

	Component
	Thread (mm)
	Torque (Nm)
	Sealer

	Flange bell fastening capscrew
	M10x1.5
	85
	 

	Flange bell fastening capscrew
	M16x2
	270
	 

	Oil sump fastening capscrew
	M8x1.25
	47
	 

	By-pass tube fastening capscrew
	M6x1
	10
	 


 






















	$MACHINE$

	$INSTRUCTION$





		Errore. Nel documento non esiste testo dello stile specificato.



	ERRORE. NEL DOCUMENTO NON ESISTE TESTO DELLO STILE SPECIFICATO.
	[image: ]





	[image: ]
	ERRORE. NEL DOCUMENTO NON ESISTE TESTO DELLO STILE SPECIFICATO.
		Errore. Nel documento non esiste testo dello stile specificato.








	EN
	4
	




	
	5
	EN



[image: C:\Users\f.filippi\Documents\job\lombardini\RETRO.png]



imgrId10406a0ec4d339a37.jpg




imgrId10946a0ec4da3b4cc.jpg




imgrId11296a0ec4d4dadb0.jpg




imgrId11386a0ec4d365c38.jpg




imgrId11626a0ec4d956768.jpg




imgrId11646a0ec4d522537.jpg
=0
~[o] [sra]

< ra
= E’?]

MIRE





imgrId12226a0ec4d9969b2.jpg




imgrId12276a0ec4d3a46fa.jpg
o
(B
-
g o8

.
.ﬂﬂuf&
ENE] ]





imgrId12456a0ec4d541fb0.jpg




imgrId12536a0ec4d9e8bb9.jpg




imgrId15556a0ec4daba145.jpg




imgrId16896a0ec4d97bb5d.jpg




image2.png
KOHLER.

IN POWER. SINCE 1920.

Lombardini s.r.. is a part of Kohler Group.
Lombardini has manufacturing facilities
in ltaly, Slovakia and India and sales
subsidiaries in France, Germany, UK, Spain
and Singapore. Kohler/Lombardini reserves
the right to make modifications without prior
notice.

www.lombardini.it

DEUTSCHLAND
Lombardini Motoren GmbH
Fritz-Klatte-Str. 6, Biirogebéude 2
D - 65933 Frankfurt

Hessen, DEUTSCHLAND

T. +49-(0)69-9508160

F. +49-(0)69-950816-30

EUROPE

Lombardini Srl

Via Cav. del lavoro

A. Lombardini n° 2

42124 Reggio Emilia, ITALY
T. +39-(0)522-389-1

F. +39-(0)522-389-503

UK

Lombardini U.K. Ltd

1, Rochester Barn - Eynsham Road
OX2 9NH

Oxford, UK

T. +44-(0)1865-863858

F. +44-(0)1865-861754

USA & CANADA

Kohler Co.

444 Highland Drive,

Kohler - Wisconsin (53044), US
T. +1 920 457 4441

F. +1 920 459 1570

ESPANA _
Lombardini ESPARA, S.L.
P.l. Cova Solera 1-9

08191 - Rubi (Barcelona)
ESPANA

T. +434-(0)9358-62111

F. +34-(0)9369-71613

FRANCE

Lombardini France S.a.s.
47 Aliée de Riottier,

69400 Limas, FRANCE

T. +33-(0)474-626500

F. +33-(0)474-623945

CHINA & ROAPAC

Kohler China INVESTMENT Co. Ltd

10.158, Jiang Chang San Road,
200436, Zhabe, Shanghai
CHINA

Tel: +86 400-0120-648

Fax: +86 21 61078904




imgrId17416a0ec4d4d2ce2.jpg




imgrId17676a0ec4d3e2e6e.jpg




imgrId18716a0ec4d771e17.gif




imgrId19486a0ec4d9a38d9.jpg




imgrId20106a0ec4d960a70.jpg




imgrId20106a0ec4da45868.jpg




imgrId20906a0ec4db47984.jpg




imgrId20966a0ec4db2a4f0.jpg




imgrId21516a0ec4d46a006.jpg




imgrId23446a0ec4d71d610.jpg




imgrId23716a0ec4d2ef9e0.jpg




imgrId24096a0ec4db212b5.jpg




imgrId24276a0ec4d9ef420.jpg




imgrId24866a0ec4db32fb0.jpg




imgrId26276a0ec4d491dba.jpg




imgrId26326a0ec4da6fd5d.jpg




imgrId27146a0ec4d39ad61.jpg
08





imgrId27756a0ec4d421bc2.jpg




imgrId27876a0ec4d96932a.jpg




imgrId28346a0ec4d6ad800.jpg




imgrId29126a0ec4d5ed3af.jpg




imgrId29366a0ec4d48dcf0.jpg




imgrId29886a0ec4d2a9be3.jpg




imgrId32096a0ec4d9b7052.png




imgrId32156a0ec4da87310.jpg




imgrId32496a0ec4d8dfbe2.jpg




imgrId32696a0ec4db2ad20.png




imgrId32956a0ec4d9ad7ac.jpg




imgrId33066a0ec4da7a758.jpg




imgrId33116a0ec4d2b5ac7.jpg




imgrId36366a0ec4d3ed104.jpg




imgrId36896a0ec4d709b13.jpg




imgrId40096a0ec4d7dde91.jpg




imgrId40166a0ec4d8a7b48.jpg




imgrId40416a0ec4d931ae4.jpg




imgrId41186a0ec4d8ea999.jpg




imgrId42476a0ec4d757c5a.jpg




imgrId42756a0ec4d673363.jpg




imgrId43446a0ec4dab4610.jpg




imgrId44546a0ec4d4c8fbe.jpg




imgrId44706a0ec4d621554.jpg




imgrId44866a0ec4d38fb56.png




imgrId45486a0ec4d52b135.jpg




imgrId45686a0ec4d43e4b2.jpg




imgrId46336a0ec4d9b6be5.jpg




imgrId46346a0ec4d899097.jpg




imgrId47146a0ec4d2cd08e.jpg
N





imgrId47686a0ec4dac1c4d.jpg




imgrId47706a0ec4da30cef.jpg




imgrId48356a0ec4da51054.jpg




imgrId48406a0ec4d551294.jpg




imgrId49526a0ec4d4e9bcf.jpg




imgrId49566a0ec4d6ef5bd.jpg




imgrId49856a0ec4d2c3e76.jpg




imgrId50216a0ec4d90c242.jpg




imgrId51166a0ec4da60ff6.jpg




imgrId51346a0ec4d382785.jpg




imgrId51516a0ec4d6bc84e.jpg




imgrId52056a0ec4d93d7a3.jpg




imgrId52616a0ec4d6d5447.jpg




imgrId54166a0ec4d9c2452.jpg




imgrId54806a0ec4d98eddc.jpg




imgrId55416a0ec4d65886c.jpg




imgrId56096a0ec4d9d3248.jpg




imgrId56916a0ec4d6f31db.jpg




imgrId58206a0ec4dac5a12.jpg




imgrId61246a0ec4d44ed48.jpg




imgrId61666a0ec4d2a2ca8.jpg




imgrId61766a0ec4d8b35bb.jpg




imgrId61846a0ec4d910c87.jpg




imgrId62786a0ec4da0a214.jpg




imgrId63076a0ec4d4c2cdd.jpg




imgrId63526a0ec4d91f217.jpg




imgrId64196a0ec4d9ddc61.jpg




imgrId64656a0ec4da56dc4.jpg




imgrId64786a0ec4d89fe9f.jpg




imgrId65756a0ec4d9cd6dd.jpg




imgrId66716a0ec4db3fc22.jpg




imgrId68306a0ec4da9da75.jpg




imgrId69976a0ec4d31a796.jpg
Vv vy
e e g e A g
IR





imgrId70136a0ec4d8c7d1b.jpg




imgrId71126a0ec4d8bfbb5.jpg




imgrId71336a0ec4da84510.jpg




imgrId72186a0ec4da81007.jpg




imgrId72806a0ec4d7b845e.jpg




imgrId73326a0ec4d58089d.jpg




imgrId74266a0ec4d89169e.jpg




imgrId74946a0ec4d357b1a.jpg




imgrId76276a0ec4d58d465.jpg




imgrId76456a0ec4d4be8e9.jpg




imgrId76996a0ec4dae9281.jpg




imgrId77386a0ec4d388522.jpg




imgrId77826a0ec4da221ec.jpg
PRERRIO
%%‘i‘f -'





imgrId77946a0ec4db0191f.jpg




imgrId79036a0ec4d83fe81.jpg




imgrId79806a0ec4da664e6.jpg




imgrId80746a0ec4d395199.jpg




imgrId81386a0ec4da17c76.jpg




imgrId82416a0ec4d98631f.jpg




imgrId82536a0ec4d73e1f5.jpg




imgrId83716a0ec4d976302.jpg
Ba





imgrId83846a0ec4d916351.jpg
m._mww

=k,




imgrId83936a0ec4d8afb9f.jpg




imgrId87266a0ec4d6cc660.jpg
b
»}





imgrId87496a0ec4d4b5155.jpg




imgrId88026a0ec4d36b4e6.jpg




imgrId88696a0ec4db152f4.jpg




imgrId89066a0ec4d5bf166.jpg




imgrId89136a0ec4d4a48e7.jpg




imgrId89336a0ec4d4993eb.jpg




imgrId90236a0ec4d4a0d6f.jpg




imgrId90566a0ec4d8d5b64.jpg




imgrId90746a0ec4d921a83.jpg




imgrId91196a0ec4d375313.jpg




imgrId91986a0ec4d34ad13.jpg




imgrId93206a0ec4d817923.jpg




imgrId93936a0ec4d6da00b.jpg




imgrId94196a0ec4d6e5653.jpg




imgrId94206a0ec4dad0a38.jpg




imgrId96366a0ec4d47b70c.jpg




imgrId96561519.jpg




imgrId96566a0ec4d32eb70.jpg




imgrId96596a0ec4d3b60f6.jpg




imgrId97756a0ec4daa8fcc.jpg




imgrId97956a0ec4da049fa.jpg




imgrId98256a0ec4d30dcd2.jpg




imgrId98666a0ec4d96e6f7.jpg




imgrId99546a0ec4da2b226.jpg




imgrId99826a0ec4da93871.jpg




image1.png
™ rehlko




