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Information about optional components

Oil dipstick in cylinder head
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	11.1.1 Check


1. Pull out the dipstick B in the direction of the arrow A .
2. Check that the mark left by the oil on the dipstick is between the MIN . and MAX . notches.
	[image: ]
Fig 11.1

	11.1.2 Replacement





11.1.2.1 Disassembly


1. Undo the screw D .
2. Pull out the oil dipstick hose E in the direction of the arrow F .
	[image: ]
Fig 11.2

	11.1.2.2 Assembly
 
[image: ]   Important
 
 
· Always replace the gasket G every time it is disassembled.


1. Insert the gasket G in the seat K of the hose E .
2. Insert the hose E in the crankcase H .






	[image: ]
Fig 11.3

	1.  Tighten the oil dipstick hose E using the screw D on the manifold L (Tightening torque of 10 Nm ).
	[image: ]
Fig 11.4

	NOTE: Check the integrity of the gaskets J.




1. Insert the dipstick B inside the hose E .
	[image: ]
Fig 11.5


 



Heater (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	11.2.1 Disassembly


1. 
Undo the screws A and the relevant washers and remove the earth cable B .
2. Remove the flange C and the manifold D .
3. Remove the heater E and the relevant gaskets F .
	[image: ]
Fig 11.6

	11.2.2 Assembly
 
[image: ]   Important
 
 
· Always replace gaskets F , with each assembly.

 
1. In sequence, fit the manifold G with the gasket F , the new heater E , the second gasket F , the flange C, the washers H , the screws A and the cable B .
2. Secure the flange H with the screws A (tightening torque at 22 Nm ).
3. Secure the earth cable B with the nut J and the relevant washer on the heater  E .
	[image: ]
Fig 11.7


 



Idler gear (for 3rd / 4th PTO)
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	11.3.1 Disassembly


1. Undo the screw A and remove the gear unit B .
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Fig 11.8

	2.   Remove the retainer ring C from the seat of the pin D .
3.   Remove the shoulder washer E , the gear B , the shoulder ring F and the bushing G from the pin D .
	[image: ]
Fig 11.9

	11.3.2 Assembly


1. Fit into the pin D :
- The shoulder ring F (of least thickness)
- The gear B
- The shoulder ring E
- The retainer ring C .
2. Insert the bushing G on the crankcase L .
	[image: ]  
Fig 11.10

	[image: ]   Important
 
 
· Always replace the washer H every time it is disassembled.
Modified component, see service letter 700019 - 700021  -  700028 .
· Check that the perforated screw A is free from impurities inside it.

 
1. Position the gear unit B on the hole J using the bushing G to centre.
2. Secure the gear B using the screw A inserting the washer H (tightening torque at see service letter 700019 - 700021  -  700028 ).
	[image: ]
Fig 11.11


 



3rd PTO (replacement)
[image: ]
Fig 11.12
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	11.4.1 Disassembly


1. Undo the screws A and remove the pump B .
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Fig 11.13

	1. Remove the centring ring C and the relative gaskets
2. Undo the screws N .
	[image: ]
Fig 11.14

	1. Remove the flange F with the components D, E , G and H in the direction of the arrow P .
2. Remove the gasket J .
	[image: ]
Fig 11.15

	1. Remove the retainer ring D and the shoulder washer E .
2. Remove the gear H and the shoulder ring G from the flange F in the direction of the arrow Q .
	[image: ]
Fig 11.16

	11.4.2 Assembly
 
[image: ]   Important
 
 
· Always replace the gasket J after each assembly.
· Lubricate the gear H with oil.
· It is mandatory to replace the screws N or apply a few beads of Loctite 2701 .


1. Insert the gear H in the flange F in the direction of the arrow R inserting the shoulder ring G .
2. Insert the shoulder ring E on the flange F and clamp the gear H using the retainer ring D .
3. Position the flange F on the crankcase K inserting the gasket J , and inserting the gear H up to the stop on the bearing L ( Fig. 11.31 ).










 
	[image: ]
Fig 11.17[image: ]


Fig 11.18

	1. Secure the flange F using the screws N (tightening torque at 25 Nm ).
 
[image: ]   Important
 
 
· Always replace the gaskets P and Q at each assembly.


1. Insert the centring ring C in the flange F up to the stop.

 
	[image: ]
Fig 11.19

	1. Insert the pump B on the flange F engaging the gear H .
2. Secure the pump B using the screws A on the flange F (tightening torque at 25 Nm ).
	[image: ]
Fig 11.20


 



4th PTO (replacement)
[image: ]
Fig 11.21
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	11.5.1 Disassembly


1. Undo the screws A and remove the pump B .
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Fig 11.22

	1. Undo the screws C and remove the flange D .
	[image: ]
Fig 11.23

	1. Undo the screws E and remove the cover F .
	[image: ]
Fig 11.24

	1. Undo the screws G and remove the flange K with the components H , J , M and N .
	[image: ]
Fig 11.25

	1. Remove the retainer ring H and the shoulder ring J from the flange K .
2. Remove the gear N and the shoulder ring M from the flange K .
	[image: ]
Fig 11.26

	11.5.2 Assembly
 
[image: ]   Important
 
 
· Always replace the shoulder ring J after each assembly.
· Lubricate the gear N with oil.
· It is mandatory to replace the screws G or apply a few beads of Loctite 2701 .


1. Insert the gear N in the flange K in the direction of the arrow W inserting the shoulder ring M .
2. Insert the shoulder ring J on the flange K and clamp the gear N using the retainer ring H .




	[image: ]
Fig 11.27

	1. Position the flange K on the crankcase Q inserting the gasket P , and insert gear N in crankcase Q .
1. Secure the flange K using the screws N (tightening torque at 25 Nm ).
	[image: ]
Fig 11.28

	[image: ]   Important
 
 
· Always replace the gasket V after each assembly.


1. Insert the gasket V on the cover F , insert and position the cover F on the flange K .
2. Secure the cover F using the screws E on the flange K (tightening torque at 25 Nm )
	[image: ]
Fig 11.29

	[image: ]   Important
 
 
· Always replace the gasket T after each assembly.


1. Position and secure the flange D using the screws C on the crankcase S (tightening torque at 10 Nm ).
	[image: ]
Fig 11.30

	[image: ]   Important
 
 
· Always replace the gasket U after each assembly.


1. Position the gasket U on the flange  D .
2. Secure the pump B using the screws A on the flange D (tightening torque at 25 Nm ).
	[image: ]
Fig 11.31


 



3rd + 4th PTO (configurations)
[image: ]
Fig. 11.32
 
	11.6.1 Information


Hydraulic pumps on the 3rd and 4th PTO can be installed at the same time.
In some configurations, there is also the centering ring C on the 4th PTO.
 
[image: ]     Important
 
 
· For disassembly or installation, refer to Par. 11.4 , Par. 11.5 e Par. 11.6 .
· Always replace the gasket of the rings B and C and flanges D and K at each assembly.
· Lubricate the gear H with oil.


	[image: ]
Fig. 11.33


 



Air filter (cartridge replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	1. Release the two hooks A and remove the cover B from the body C .
2. Remove the cartridges D .
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Fig 11.34

	1. Insert the new cartridge D and both of them inside the filter body C .
2. Secure the cover B via the hooks A .
	[image: ]
Fig. 11.35


 



Remote oil filter (disassembly and assembly)
	 
[image: ] Important
 
 
· Modified component, see service letter 700018 .




11.9.1 Disassembly


1. Perform the operations described in Par. 5.2 .

 
[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
· For the replace the cartridge, please refer to operation number 6 (Par. 11.9.1) and 2 (Par. 11.9.2) .
· For the disassembly of the pipes B and C, lock with a tool the fittings K, H (Fig. 11.37) and L (Fig. 11.38) in order to prevent their lose together with the nuts A , with the consequent of oil leakage.
1. Undo the nuts A and remove the hoses B and C .
	[image: ]
Fig 11.36

	1. Release the clamps D and remove the hoses E and F from Oil Cooler G .
2. Unscrew and remove the fitting H with its copper gasket from the oil filter head J .
3. Unscrew and remove:
    - the fitting K with the copper gasket;
    - Oil Cooler G and the relative gaskets;
    - the oil filter head J .
	[image: ]
Fig 11.37

	1. Unscrew the fittings L and remove the copper gaskets from the support M .
2. Unscrew the cartridge N with gasket from the support M .
	[image: ]
Fig 11.38

	11.9.2 Assembly

 
 
[image: ]   Important
 
 
· Always replace the gaskets V after each assembly.
· Always replace the gaskets P, Q, and U at each assembly.
· Lubricate the gaskets P, Q with oil before assembling them.




1. Clamp unions L on support M inserting  gasket V (tightening torque at 40 Nm ).
2. Lubricate gasket W and clamp cartridge N on support M (tightening torque at 20 Nm ).
3. Insert the gasket P on the seat of the fitting K .
4. Insert flange head J on the union K and the gasket Q in the seat of head J .
5. Insert the Oil Cooler G on the union K and the gasket R in the seat of Oil Cooler G .
6. Onto crankcase S apply Oil Cooler G and flange J by means of union K (tightening torque at 25 Nm + Loctite 2701 on thread) as positioned in Fig. 11.39 .
7. Clamp union H on flange J inserting gasket U (tightening torque at 40 Nm ).
	[image: ]
Fig 11.39

	1. Connect the hose B to the central fitting of support M and of flange J .
2. Connect the hose C to the side fitting of the support M and of head J .
3. Clamp the nuts A on the head J (tightening torque at 30 Nm ).
4. Clamp the nuts A on the support M (tightening torque at 35 Nm ).
 
[image: ]   Important
 
 
· Check the tightening of the fittings K, H (Fig. 11.37) and L (Fig. 11.38) (tightening torque at 40 Nm ).


	  [image: ]
Fig 11.40


 



Poly-V alternator belt (replacement and adjustment)
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	1. Loosen the nut B and manually tighten the screw C until it just touches the pulley pin D .
	[image: ]
Fig 11.41

	1. Untighten the screw E by around 32mm (A) .
2. Untighten the screw C .

 
NOTE: The belt tensioner pulley F should move towards the arrow G . If it does not, please move it manually.
	[image: ]
Fig 11.42

	1. Remove the V-Belt H and install the new one.

 
NOTE: Ensure that the internal profile of belt H is properly inserted into the grooves of the pulley A (as illustrated in D1 e D2 ).
	[image: ]
Fig 11.43

	1. Tighten capscrew C , to shift gudgeon D fully to the bottom of the grooved guide.
2. Tighten capscrew E (tightening torque at 45Nm ).
3. Hold the screw C still with a key, and tighten the screw B on the plate L to secure the screw C (tightening torque at 45Nm ).
4. Check, in point  P  the tension of the belt. 
 
[image: ]    Important
 


· Modified component, see service letter 700037.
	[image: ]
Fig 11.44


 



Tightening pulley and alternator for Poly-V belt
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
	 

	11.4.1 Disassembly


1. Perform the operations from point 1 to 3 of Par. 11.9.
2. Remove the belt H ( Fig. 11.43 ) .
3. Undo and remove the screw A .
4. Fully undo the screw B and remove the tightening pulley C .
	[image: ]
Fig 11.45

	1. Undo the screws D and remove the plate E and the pin F .
	[image: ]
Fig 11.46

	1. Undo the screws G and H remove the alternator L .
	[image: ]
Fig 11.47

	1. Undo the screws M and remove the bracket N .
	[image: ]
Fig 11.48

	11.4.2 Assembly


1. Secure the bracket N using the screws M on the cylinder head P (tightening torque at 25 Nm ).
	[image: ]
Fig 11.49

	1. Insert the screw H into the fixing hole on the alternator L .
2. Insert the spacer R on the screw H (between the alternator and crankcase).
3. Tighten the screw manually H onto the crankcase Q .
4. Orientate the second fixing hole of the alternator L with the hole of the bracket N , secure the alternator L using the screw G (tightening torque at 25 Nm ) onto the bracket N and then the screw H (tightening torque at 25 Nm ).
	[image: ]
Fig 11.50

	1. Insert the pin F in the plate slot E .
2. Orientate the pin F with the surface S (support for screw A ) upwards.
3. Secure the plate E using the screws D on the bracket N (tightening torque at 25 Nm ).
	[image: ]
Fig 11.51

	1. Insert the screw B in the plate C1 and pulley C .
2. Manually tighten the screw B onto the pin F up to the stop; Undo the screw B again by one turn.

 
NOTE: The screw B must protrude by about 32 mm (A) from the surface of the tightening pulley C (see detail X ).

 
3. Install the new belt H ( Fig. 11.43 ) .
4. Tighten the screw A onto the plate E up to the stop on the pin F .
5. Perform the operations point 6 to 8 of Par. 11.9 .
	[image: ]
Fig 11.52


 



Oil sump with supporting structure
	11.11.1 Flywheel (J) disassembly


1. Execute the operations described in Par. 7.11.1 .




11.11.2 Plate/flange housing (L) disassembly


1. Loosen supplementary capscrews A and B .
2. Execute the operations described in Par. 7.11.2 .
3. Remove housing or plate L .
	[image: ]
Fig. 11.53



	11.11.3 Oil sump disassembly


1. Execute the operations described in Par. 5.2 .
2. Loosen capscrews C and remove bypass tube D .
3. Loosen capscrews E and remove oil sump F .
	[image: ]
Fig. 11.54



	11.11.4 Oil sump assembly


1. Make sure contact surfaces G of oil sump F and crankcase H have no impurities.
2. Apply a sealing bead of approximately 2.5 mm ( Loctite 5660 ) onto surface G of crankcase H .
3. Place oil sump F onto crankcase H in correspondence with the fastening holes (use tool ST_18 ).
	[image: ]
Fig. 11.55



	[image: ]
Fig. 11.56



	1. Apply capscrews E into the fastening holes and use torque at 10 Nm .
2. Loosen capscrews E , leaving approximately 1 mm leeway ( position A ) between the neck surface of capscrews E and oil sump F .
3. Place flange housing or plate L onto crankcase H , complying with centring tap pins M .
4. Using 2 capscrews A , fasten housing or plate L onto crankcase H (tightening torque at  20 Nm ).
5. Using 2 capscrews A , fasten housing or plate L onto oil sump F (tightening torque at 20 Nm ).
	[image: ]
Fig. 11.57



	[image: ]

  Fig. 11.58



	1. Fasten oil sump F by tightening capscrews E and strictly following the order shown in Fig. 11.59 (tightening torque at  20 Nm ).
2. Loosen capscrews A and remove housing or plate L ( Fig. 11.58 ).
3. Fasten oil sump F by tightening capscrews E and strictly following the order shown in Fig. 11.59 (tightening torque at  47 Nm ).
Loosen the screw 1 again and tighten it to 47 Nm .
	[image: ]
Fig. 11.59



	1. Insert gaskets N into seats P of bypass tube D .
2. Fasten bypass tube D onto oil sump F using capscrews C (tightening torque at 10 Nm ).
	  [image: ]
Fig. 11.60



	11.11.5 Flange plate / housing assembly


1. Execute the operations described in point 6 of Par. 11.11.4 .
2. Fasten housing or plate L by using capscrews A and strictly following the order shown in Fig. 11.61 (tightening torque at 85 Nm ).
3. Fasten housing or plate L by using capscrews B (tightening torque at 270 Nm ).


11.11.6 Flywheel assembly


1. Execute the operations described in Par. 9.5.2 .
	[image: ]
Fig. 11.61
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