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Information about optional components

Heater (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.1.1 Disassembly


1. Undo the screws A .
2. Remove the flange C .
3. Remove the heater E and the relevant gaskets F .
	[image: ]
Fig 11.1

	11.1.2 Assembly
 
[image: ]   Important
 
 
· Always replace gaskets F , with each assembly.

 
1. In sequence, fit the manifold G with the gasket F , the new heater E , the second gasket F , the flange C , the washers H , the screws A and the cable B .
2. Secure the flange C with the screws A (tightening torque at 22 Nm ).
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Fig 11.2


 



Idler gear (for 3rd / 4th PTO)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.2.1 Disassembly


1. Perform the operations of point 7 of Par. 7.4.1 .
2. Perform the operations from point 2 to 3 of  Par. 6.6.1 .
3. Perform the operations of point 3 of  Par. 7.8.1 .
4. Perform the operations of Par. 7.8.2 .
5. Loosen capscrews A and remove plate B1 .
6. Extract gear C .
7. Remove gudgeon D together with plate B2 .
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Fig 11.3
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Fig 11.4

	11.2.2 Assembly
 
[image: ]   Important
 
 
· Make sure that gudgeon D has no impurities inside.

 
1. On capscrew A , assemble:

    - plate B1
    - gudgeon D
    - gear C  
    - plate B2 .
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Fig 11.5



	1. Position gear unit C1 onto crankcase E , complying with reference J1 , J2 with gear F .
2. Secure unit C1 by means of capscrew A (tightening torque 25 Nm ).
NOTE: the reference J1 can have 2 different configurations for the gear C , Fig. 11.6b shows the correct position of the reference J1 for both configurations.
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Fig 11.6
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Fig 11.6b




 



3rd PTO (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.3.1 Disassembly


1. Perform the operations of point 7 of  Par. 7.4.1 .
2. Perform the operations from point 2 to 3 of  Par. 6.6.1 .
3. Perform the operations of point 3 of Par. 7.8.1 .
4. Perform the operations of Par. 7.8.2 .
5. Extract gear A .
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Fig 11.7

	11.3.2 Assembly


1. Insert gear A into the seat of crankcase B , fitting the shaft of pump C in gear A .
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Fig 11.8


 



4th PTO (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.4.1 Disassembly


1. Perform the operations of point 7 of  Par. 7.4.1 .
2. Perform the operations from point 2 to 3 of  Par. 6.6.1 .
3. Perform the operations of point 3 of Par. 7.8.1 .
4. Perform the operations of Par. 7.8.2 .
5. Extract gear A .
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Fig 11.9

	11.4.2 Assembly


1. Insert gear A into the seat of crankcase B , fitting the shaft of pump C in gear A .
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Fig 11.10


 



Balancer device (replacement)
	[image: ]   Importante
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.5.1 Disassembly


1. Perform the operations described in Par. 11.2.1 .
2. Extract shaft A1 e A2.
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Fig 11.11

	11.5.2 Assembly


1. Lubricate gudgeon C of shaft A1 and A2 with oil.
2. Insert shaft A1 into seat B1 of the crankcase, complying with reference D of gear E .
3. Insert shaft A2 into seat B2 of the crankcase.
4. Perform the operations described in Par. 11.2.2 .
NOTE: the shafts A1 and A2 are different and it is important not to invert the assembly position, the reference D is specific for the shaft A1 and is timed with the gear E , the reference J2 is specific for the shaft A2 and is timed with the idler gear F (see the Fig. 11.12b ).
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Fig 11.12
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Fig 11.12b




 



ETB (replacement)
	1. Unscrew screws A and remove the ETB valve B with its gasket C . 
 
[image: ]   Important
 
 

 

· Always replace the gasket C  at each assembly.
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Fig. 11.13

	1. Fix the ETB valve B and its gasket C by means of screws A (tightening torque 10 Nm )
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Fig. 11.14
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