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Information for disassembly

Recommendations for disassembly
 
[image: ]     Important
 
 
· The mark ( [image: ] ) after the title of a paragraph, indicates that the procedure is not required in order to disassemble the engine, however the procedures are featured in order to illustrate the disassembly of components.
· The operator should prepare all equipment and tools in order to enable him to carry out the operations correctly and safely.
· Before disassembly, perform the operation described in Chap. 5 .
· Before proceeding with operation, carefully read Chap. 3 .
· In order to operate safely and easily, we recommend positioning the engine on a rotating stand for engine overhauling.
· Seal all injection component unions as illustrated in Par. 2.9.8 during assembly.
· Protect all disassembled components and coupling surfaces subject to oxidation with lubricant.
· Where necessary, reference to special tools to use during disassembly operations is indicated (es. ST_05 ), identified in Tab. 13.1 - 13.2 - 13.3 .



EGR circuit disassembly
	7.2.1 EGR cooler unit


1. Undo the screws A ( ST_06 ) and B and remove the pipe C with the relative gaskets.
	[image: ]
Fig 7.1

	1. Undo the screws D, E ( ST_06 ) and remove pipe F and the relevant gaskets.
	[image: ]
Fig 7.2

	1. Release the clamp M and remove pipe N .
2. Release the clamp L .
3. Undo capscrews G and remove EGR Cooler H from hose X ( ST_05 ) .
	[image: ]
Fig 7.3

	7.2.2 EGR Valve
1. 


Disconnect the connector P .
2. Undo the screws Q and remove the EGR valve R with the relevant gasket.

 
NOTE: The EGR valve is not a serviceable item, and if damaged/worn, it should be replaced with a new one.
	[image: ]
Fig 7.4

	1. Undo capscrews S and remove flange T with the relative gasket.
	[image: ]
Fig 7.5


 



Electric components disassembly
	7.3.1 Electric wiring

 
[image: ]   Important
 
 
· Refer to Par. 2.13 prior to proceeding with disassembly.


1. Disconnect the connectors  A, B and C .
2. Release the clamp D .
	[image: ]
Fig 7.6

	1. Disconnect the connectors E, F and G .
2. Release the clamps J and H .
	[image: ]
Fig 7.7

	1. Disconnect the connectors K and L .
	[image: ]
Fig 7.8

	1. Disconnect the connectors M and P .
2. Release the clamp Q .
	[image: ]
Fig 7.9

	1. Disconnect the connectors R .
2. Undo the screws S and remove the wiring support T ( ST_06 ) .
	[image: ]
Fig 7.10

	7.3.2 Starter motor

 
[image: ]   Important
 
 
· The motor is not repairable.


1. Undo the screws U and remove the starter motor V .
	[image: ]
Fig 7.11

	7.3.3 Belt and alternator
1. 


Loosen the screws Z and W .
2. Push the alternator AA in the direction of the arrow AB .
3. Remove the belt AC from the pulleys AR .
4. Undo the screws Z and W and remove the alternator AA .


 
[image: ]   Important
 
 
· The belt must always be replaced every time it is disassembled, even if it has not reached the scheduled hours for replacement.
	[image: ]
Fig 7.12

	7.3.4 Sensors and switches

 
[image: ]   Important
 
 
· After disassembly, protect the sensors suitably against knocks, dampness and any high temperature sources.
· The sensors and switches cannot be repaired, therefore they must be replaced in the event of anomalies.

 
7.3.4.1 Oil pressure switch ( [image: ] )
1. 


Unscrew and remove the oil pressure switch AD .
	[image: ]
Fig 7.13

	7.3.4.2 Coolant temperature sensor ( [image: ] )
1. 


Unscrew and remove the coolant temperature sensor AE .
	[image: ]
Fig 7.14

	7.3.4.3 Speed sensor ( [image: ] )
1. 


Undo the screw AF and remove the sensor AG with the relative spacer ( ST_06 ) .
2. Undo the screws AH and remove the sensor ( ST_06 ) .
	[image: ]
Fig 7.15

	7.3.4.4 Camshaft phase sensor
1. 


Undo the screw AM and remove the sensor AN with the relative spacer ( ST_06 ).
	[image: ]
Fig 7.16

	7.3.4.5 T-MAP Sensor ( [image: ] )


1. Undo the screw AP and remove the sensor AQ ( ST_06 ).
	[image: ]
Fig 7.17

	7.3.4.6 Fuel filter water detection sensor ( [image: ] )

 
[image: ]   Warning
 
 
· The fuel filter is not always mounted on the engine.
· When disassembling the sensor A , use a suitable container to recover the fuel contained in the cartridge B .

 
1. Unscrew the sensor A from the cartridge B .
	[image: ]
Fig 7.18


 



Turbocharger disassembly
	1. Release the clamps A and B and remove the manifold C .
	[image: ]
Fig 7.19

	1. Unscrew the fittings D and remove the pipe E with the relative gaskets G .
2. Undo the screws F .
3. Release clamp M .
	[image: ]
Fig 7.20

	1. Undo the nuts L .
2. Remove tube N .
	[image: ]
Fig 7.21





Exhaust manifold disassembly
	1. Undo the nuts A and remove the manifold B and the gaskets C .
2. Close the openings and manifolds to prevent foreign bodies from entering.
	[image: ]
Fig 7.22


 



Coolant recirculation components disassembly
	7.6.1 Oil Cooler manifold


1. Release the clamps Z .
2. Undo the screw W and remove hoses J ( ST_05 ) .
	[image: ]
Fig 7.23

	1. Release the clamp K and remove hoses AA .
	[image: ]
Fig 7.24

	7.6.2 Coolant pump
 
[image: ]     Important
 
 
· The pump B is not repairable.


1. Undo the screws A and remove the water pump unit B with its gasket C .
	[image: ]
Fig 7.25

	7.6.3 Thermostatic valve
1. 


Undo the screws A and remove the thermostatic valve cover B .
2. Remove the thermostatic valve C and its gasket.

 
 
 
[image: ]     Important
 
 
· Always replace the gasket D every time it is disassembled.


1. Check that the air bleeding hole is not clogged or blocked ( Par. 2.11.4 ).
	[image: ]
Fig 7.26


 



Crankshaft and target wheel pulley disassembly
	1. Position the crankshaft with the 1st cylinder at TDC,reference H .
2. Undo the screw C clockwise.
3. Remove the drive pulley unit and the target wheel D .
	[image: ]
Fig 7.27


 



Lubrication circuit disassembly
	7.8.1 Oil pressure valve( [image: ] )


1. Undo the cap A .
2. Remove the spring B , check its condition and replace it if broken.
3. Remove the valve piston C using a magnet.
	[image: ]
Fig 7.28

	7.8.2 Timing system carter oil filling flange ( [image: ] )


1. Undo the screws D and remove the oil filling flange E ( ST_06 ) .
2. Remove the gasket F .
	[image: ]
Fig 7.29

	7.8.3 Timing system carter


1. Ensure that the crankshaft with the 1st cylinder is at the TDC (taper pin W must be facing upwards).
2. Undo the screws G .
3. Remove the timing system semi-crankcase H .
	[image: ]
Fig 7.30

	7.8.4 Oil pump

 
[image: ]   Important
 
 

 

· The oil pump is not repairable.

 
1. Undo the screws L and remove the pump unit M from the timing system carter H ( ST_06 ) .
	[image: ]
Fig 7.31

	1. Remove the rotors N and P from oil pump carter M .
	[image: ]
Fig 7.32

	7.8.5 Oil Cooler unit and lub. oil filter
1. 


Screw the lid cartridge holder V .
2. Undo the screws Q, R and remove Oil Cooler group S .

 
 
[image: ]     Warning
 
 
· Use a suitable container to recover any residue oil.
· Oil Cooler unit S is not repairable.
	[image: ]
Fig 7.33

	1. Remove the gaskets T and U .

 
NOTE: To replace the oil cartridge, refer to Par. 6.10.2 .
	[image: ]
Fig 7.34

	7.8.6 Oil vapour separator unit


1. Release the clamps AA .
2. Remove the manifolds AB, AC and AD .
3. Remove the clamp AE by carefully cutting it at the point indicated and remove the oil separator AF .
	[image: ]
Fig 7.35

	1. Undo the screws AG .
2. Remove la flangia di supportoRemove flange support AH and the gasket seal AL .
	[image: ]
Fig 7.36


 



Intake manifold disassembly
	1. Undo the screws A and remove the semi-manifold B ( ST_05 ) .
2. Remove the separation plate C and the gaskets H .
	[image: ]
Fig 7.37

	1. Undo the screws D ( ST_06 ) and E .
2. Remove the semi-manifold F and the gasket G .
	[image: ]
Fig 7.38


 



Fuel system disassembly
	7.10.1 Fuel return pipes


1. 
Release the clip A .

 
 
[image: ]     Warning
 
 
· After removing the union, the clip A must automatically return to its initial position; otherwise it must be replaced.




1. Undo the B distributor return fixing capscrew.
2. Release the clamp D .
3. Disconnect the pipe E from the fuel return fitting.
4. Undo and remove the screw G with the relative gaskets and put the cap on the Common Rail pressure relief valve AA .
5. Disconnect unions M from electronic injectors N .
6. Remove the fuel return pipes.
	[image: ]
Fig 7.39[image: ]


Fig 7.40

	7.10.2 Fuel flow pipes
 
[image: ]   Important
 
 

 

· Seal all openings of the inlet and return unions on the injection pump D with the relevant caps, in order to prevent impurities from entering.

 
1. Loosen the clamps P .
2. Remove the pipes Q and R .
	[image: ]
Fig 7.41

	7.10.3 High pressure fuel pipes

 
[image: ]     Danger
 
 
· The fuel injection circuit undergoes high pressure, use safety protections as described in Par 3.4.3 .
· Ensure that the Common Rail is not under pressure by slowly and carefully unscrewing one of the nuts S .

 
1. Loosen the nuts S and T in sequence.
2. Fully undo the nuts S and T in sequence, and remove the high pressure pipes U and V .
	[image: ]
Fig 7.42

	7.10.4 Common Rail
1. 


Undo the screws AB and remove the Common Rail AC .

 
NOTE: Take care to protect te sensor AD from knocks, moisture and any high temperature source. The internal parts of the rail cannot be repaired.

 
[image: ]     Important
 
 
· Seal all injection component unions as illustrated in Par. 2.9.8 .
· Common rail cannot be repaired.
	[image: ]
Fig 7.43

	7.10.5 Electronic injectors

 
[image: ]     Important
 
 
· In the event that the electronic injectors are disassembled (not necessarily replaced), mark them with the relevant cylinder number from which they originate so as not to confuse them during re-assembly (Fig. 7.45) .
· The electronic injectors cannot be repaired.
· If one or more electronic injectors are to be replaced, the new calibration data must be inserted in the ECU via a specific instrument ( ST_01 ).
· Be careful not to damage the gaskets X .

 
1. Undo capscrews AE and remove them together with the relative washers AF and then brace AG .
2. Pull out the electronic injector AH .

 
NOTE: Should you be unable to remove the electronic injector (acting only on point BC ), use an open-ended spanner (Ø 34 mm), by applying small rotations to unblock the component.

 
3. Seal all injection component unions as illustrated in Par. 2.9.8 .
4. Ensure that gasket AL has remained in the correct position (Fig. 7.46) .
Otherwise, recover the gasket from inside the electronic injector AM .
	[image: ]
Fig 7.44[image: ]


Fig 7.45

	7.10.6 Fuel filter ( [image: ] )
1. 


Undo the fuel cartridge AW from support AP .
2. Undo the screws AN and remove the filter support AP .
	[image: ]
Fig 7.46

	7.10.7 High-pressure fuel injection pump

 
[image: ]   Important
 
 
· Before disassembling, carefully read Par. 2.17 .
· The injection pump is not repairable
· Should the fuel feeding pump need to be replaced, after assembly, it is necessary to perform the Pump Learning procedure by means of instrument ST_01 .

 
1. Undo the nut AQ .
2. Loosen the screws AR of the injection pump.
3. Screw the tool ST_04 on the thread of the gear AS .
4. Tighten the screw AT on the puller to disconnect the gear AS from the injection pump and remove the injection pump control gear AS .
5. Undo the screws AR .
6. Remove injection pump AU   and the relative gasket AV .
7. Seal all injection component unions as illustrated in Par. 2.9.8 .
	[image: ]
Fig 7.47[image: ]


Fig 7.48


 



Timing system gear disassembly
	1. Unscrew screws H and remove target wheel G .
2. Unscrew screws D and remove camshaft gear E .
3. Remove retainer ring A and the shoulder ring B .
4. Remove the intermediate gear C .
	[image: ]
Fig 7.49

	1. Remove the shoulder ring F .
2. Unscrew the screws L and remove the intermediate gear support M .
	[image: ]
Fig 7.50


 



Flange unit disassembly
	7.12.1 Flywheel

 
[image: ]   Important
 
 
· Leave the special tool ST_34 for blocking the flywheel ( Par. 7.7 ) .


1. Only undo the screw C located uppermost.
2. Insert the tool ST_09 in the seat of the screw C tightening it all the way.
3. Undo the remaining screws D .

 
 
[image: ]   Danger
 
 
· The flywheel E is very heavy. Pay the utmost attention while removing it in order to prevent it dropping or falling, as this may have serious consequences for the operative.


1. Remove the flywheel E .
2. Remove the tool ST_09 .
3. Remove the tool ST_34 shown in Fig. 7.11 .
	[image: ]
Fig 7.51

	7.12.2 Flange housing
1. 


Undo the screws A and remove the engine housing B .

 
 
[image: ]   Danger
 
 
· The flange housing is very heavy. Pay the utmost attention while removing it in order to prevent it dropping or falling, as this may have serious consequences for the operative.
	[image: ]
Fig 7.52


 



Cylinder head unit disassembly
	7.13.1 Rocker arms cover
1. 


Undo the screws A .
2. Remove the rocker arms cover B .
3. Remove the gasket C .
	[image: ]
Fig 7.53

	7.13.2 Rocker arm pin
1. 


Undo the screws D .
2. Remove the rocker arm pin unit E .
	[image: ]
Fig 7.54

	7.13.2.1 Rocker arm ( [image: ] )
1. 


Remove the retainer ring F .
2. Remove the shoulder rings G .
3. Remove the rocker arms H .
	[image: ]
Fig 7.55

	7.13.3 Valve rods and bridges
1. 


Remove the valve control U-bolts M .
2. Remove the rocker arm control rods N .
	[image: ]
Fig 7.57

	7.13.4 Cylinder head

 
[image: ]   Important
 
 
· The cylinder head fastening bolts P must be replaced every time they are disassembled.


1. Undo the bolts P .

 
 
 
[image: ]   Important
 
 
· To lift cylinder head Q , only use both eyebolts AE provided by KOHLER (refer to Fig. 7.66 ).
· When removing the cylinder head Q and subsequent disassembly, control, and assembly operations, it is necessary to protect the contact surface W of cylinder head Q and crankcase J against impacts.


1. Remove the cylinder head Q .
2. Remove the head gasket R .
	[image: ]
Fig 7.58[image: ]


Fig 7.59

	7.13.4.1 Valves ( [image: ] )
1. 


Mount the tool ST_07 on the head AF fixing it on one of the holes for fixing the rocker arm cover.

 
NOTE: Change the fixing hole according to the position of the valves to be removed.

 
2. Position the tool ST_07 on the valve as shown in the figure.
	[image: ]
Fig 7.60

	1. Push the lever of the tool ST_07 downwards, in order to lower the valve plates S in the direction of the arrow T , remove cotters U using a magnet.
NOTE: Repeat all the operations for all the valves concerned.
	[image: ]
Fig 7.61

	[image: ]     Important
 
 
· Before removing the valves, make some marks to record their original position, in order to avoid confusing them when reassembling (if they are not replaced).


1. Remove the valves V .
	[image: ]
Fig 7.62

	7.13.4.2 Electronic injector sleeves ( [image: ] )
1. 


Unscrew and remove the sleeves Z from the head Q .
2. Remove the gaskets AA and AB .
	[image: ]
Fig 7.63

	7.13.4.3 Valve stem gasket ( [image: ] )
1. 


Remove the gaskets AC .
	[image: ]
Fig 7.64

	7.13.4.4 Lifting eyebolts ( [image: ] )
1. 


Undo the screws AD and remove the eyebolts AE .
2. Thoroughly wash the cylinder head Q .
	[image: ]
Fig 7.65


 



Oil sump unit disassembly
	7.14.1 Oil sump
1. 


Undo the screws A .
2. Remove the oil sump B by inserting a plate in the areas indicated by the arrow AA .
	[image: ]
Fig 7.66

	7.14.2 Oil suction pipe
1. 


Undo the screws C and remove the oil pipe D .
	[image: ]
Fig 7.67

	7.14.3 Oil vapour pipes ( [image: ] )
1. 


Unscrew and remove the pipes E .
	[image: ]
Fig 7.68


 



Engine block disassembly
	7.15.1 Crankshaft gasket flange
1. 


Undo the screws A .
2. Remove the flange B and the gasket C .
	[image: ]
Fig 7.69

	7.15.2 Piston unit/connecting rod

 
[image: ]     Important
 
 
· Mark some numerical references (cylinder n°) on the connecting rods, connecting rod caps F1 , pistons and gudgeon pins to prevent unintentionally confusing the components not replaced during assembly. Failure to do this may result in engine malfunctions.
· References on connecting rod M and cap F1 must only be carried out on a side in correspondence with K1 and K2 , as illustrated in Fig. 7.70a .


1. Screw the bolt AM temporarily.
2. Unsrew bolts E1 and remove the connecting rod caps F1 .
	[image: ]
Fig 7.70







	NOTE : coupling cap F1 on the connecting rod can be carried out with centring taper pins (Fig. 7.70b) or broken ( Fig. 7.70c - without centring taper pins).
 


[image: ]
Fig. 7.70b




[image: ]
Fig. 7.70c


	

[image: ]
Fig 7.70a  



	
1. Pull out the connecting rod - piston assembly from position 2 and 3 by manually applying pressure on the connecting rod big end L in the direction of arrow AK .
2. Couple the connecting rod big end caps L with the relevant piston and connecting rod unit M .
3. Turn capscrew AM and rotate the crankshaft by 180°.
4. Repeat points 2 to 5 to disassemble the connecting rod-piston assembly to position 1 and 4 .
	[image: ]
Fig 7.71

	 
 
[image: ]     Warning
 
 
· The connecting rod half-bearings Z are made of special material. Therefore, they must be replaced every time they are removed to prevent seizures.
	[image: ]
Fig 7.72

	7.15.3 Lower semi-crankcase

3 CYLINDERS
1. 

Undo capscrews E and F by following the order indicated in the figure.
2. Remove the lower semi-crankcase D and store it in a suitable container for washing.
	 3 Cylinders
[image: ]
Fig 7.73

	4 CYLINDERS
1. 

Undo capscrews E and F by following the order indicated in the figure.
2. Remove the lower semi-crankcase D and store it in a suitable container for washing.
	 4 Cylinders
[image: ]
Fig 7.74

	7.15.4 Crankshaft


Remove:

1. Crankshaft G .
2. The shoulder semi-rings H .
	[image: ]
Fig 7.75

	7.15.5 7.15.5 Piston ( [image: ] )
1. 


Remove the retainer ring N .
2. Remove the pin P to separate the piston Q from the connecting rod R .

 
 
[image: ]   Important
 
 
· If they are not replaced, keep the components together (connecting rod - piston - gudgeon pin) by using references in order to prevent them from getting mixed up during assembly.
	[image: ]
Fig 7.76

	7.15.5.1 Rings ( [image: ] )
1. 


Remove the rings S .
	[image: ]
Fig 7.77

	7.15.6 Oil spray nozzles ( [image: ] )
1. 


Undo the screws T and remove the spray nozzles U from the upper semi-crankcase AB .
	[image: ]
Fig 7.78

	7.15.7 Camshaft
1. 


Remove the lock ring V .
2. Extract the camshaft W from the upper semi-crankcase AB .
	[image: ]
Fig 7.79

	7.15.8 Camshaft tappets
1. 


With a magnet, remove the tappets AA from the upper semi-crankcase AB .
	[image: ]
Fig 7.80

	7.15.9 Crankshaft bushings


1. Remove the crankshaft bushings AC from the upper crankcase AB .
 
[image: ]   Important
 
 

 

· The crankshaft half-bearings AC are made of special material. Therefore, they must be replaced every time they are removed to prevent seizures.
	[image: ]
Fig 7.81

	1. Remove the crankshaft bushings AF from the lower semicrankcase AE .
	[image: ]
Fig 7.82

	7.15.10 Cover 3 th PTO ( [image: ] )
1. 


Undo the screws AG .
2. Remove the cover AH and the gasket AL from the semicrankcase top.
	[image: ]
Fig 7.83


 






















	$MACHINE$

	$INSTRUCTION$





		Errore. Nel documento non esiste testo dello stile specificato.



	ERRORE. NEL DOCUMENTO NON ESISTE TESTO DELLO STILE SPECIFICATO.
	[image: ]





	[image: ]
	ERRORE. NEL DOCUMENTO NON ESISTE TESTO DELLO STILE SPECIFICATO.
		Errore. Nel documento non esiste testo dello stile specificato.








	EN
	4
	




	
	5
	EN



[image: C:\Users\f.filippi\Documents\job\lombardini\RETRO.png]



imgrId10176a452e25cb6d4.gif




imgrId10176a452e28a400b.gif




imgrId10816a452e266663a.jpg




imgrId11146a452e285e7d1.png




imgrId11336a452e2719e75.jpg




imgrId11886a452e26d524c.jpg




imgrId14356a452e25264f7.jpg




imgrId15016a452e269b402.jpg




imgrId15156a452e2780d46.gif




imgrId15766a452e255fa10.jpg




image2.png
KOHLER.

IN POWER. SINCE 1920.

Lombardini s.r.. is a part of Kohler Group.
Lombardini has manufacturing facilities
in ltaly, Slovakia and India and sales
subsidiaries in France, Germany, UK, Spain
and Singapore. Kohler/Lombardini reserves
the right to make modifications without prior
notice.

www.lombardini.it

DEUTSCHLAND
Lombardini Motoren GmbH
Fritz-Klatte-Str. 6, Biirogebéude 2
D - 65933 Frankfurt

Hessen, DEUTSCHLAND

T. +49-(0)69-9508160

F. +49-(0)69-950816-30

EUROPE

Lombardini Srl

Via Cav. del lavoro

A. Lombardini n° 2

42124 Reggio Emilia, ITALY
T. +39-(0)522-389-1

F. +39-(0)522-389-503

UK

Lombardini U.K. Ltd

1, Rochester Barn - Eynsham Road
OX2 9NH

Oxford, UK

T. +44-(0)1865-863858

F. +44-(0)1865-861754

USA & CANADA

Kohler Co.

444 Highland Drive,

Kohler - Wisconsin (53044), US
T. +1 920 457 4441

F. +1 920 459 1570

ESPANA _
Lombardini ESPARA, S.L.
P.l. Cova Solera 1-9

08191 - Rubi (Barcelona)
ESPANA

T. +434-(0)9358-62111

F. +34-(0)9369-71613

FRANCE

Lombardini France S.a.s.
47 Aliée de Riottier,

69400 Limas, FRANCE

T. +33-(0)474-626500

F. +33-(0)474-623945

CHINA & ROAPAC

Kohler China INVESTMENT Co. Ltd

10.158, Jiang Chang San Road,
200436, Zhabe, Shanghai
CHINA

Tel: +86 400-0120-648

Fax: +86 21 61078904




imgrId17606a452e2802e54.jpg




imgrId17786a452e2795b5b.jpg




imgrId17796a452e263d48a.jpg




imgrId18356a452e27e3f67.gif




imgrId18746a452e277ce5c.jpg




imgrId18936a452e28184c9.jpg




imgrId19616a452e272ccc6.jpg




imgrId19736a452e25dfdd4.jpg




imgrId20016a452e2693eea.jpg




imgrId21346a452e282bb1d.jpg




imgrId23006a452e265eb5b.jpg




imgrId23676a452e2621317.jpg




imgrId25286a452e2656b86.gif




imgrId28546a452e258c17b.jpg




imgrId29136a452e2706c8d.jpg




imgrId29526a452e2596c2c.gif




imgrId30626a452e259c3f8.jpg




imgrId30836a452e2671d6b.jpg




imgrId30986a452e27eb775.jpg




imgrId33106a452e27de44d.jpg




imgrId33686a452e25580d1.jpg




imgrId33736a452e2647688.jpg




imgrId37716a452e288213b.jpg




imgrId38106a452e2579bd9.jpg




imgrId39166a452e272537e.gif




imgrId41406a452e26c3f48.jpg




imgrId41726a452e2740198.jpg




imgrId42876a452e2551b70.jpg




imgrId42916a452e2821f14.jpg
4

|
.
|” o g

e




imgrId43036a452e25cfacc.jpg




imgrId43836a452e28dc50e.jpg




imgrId44556a452e25c6c04.jpg




imgrId44596a452e28a0e2e.jpg




imgrId45156a452e26ab239.jpg




imgrId45346a452e275e645.jpg




imgrId45486a452e26d85be.jpg




imgrId48176a452e26b3602.jpg




imgrId48616a452e2875092.jpg
W
V.





imgrId48936a452e264b60c.gif




imgrId49046a452e27309c9.jpg




imgrId49646a452e28c2a2f.jpg




imgrId49706a452e251712e.jpg




imgrId49796a452e25a18d4.gif




imgrId50366a452e2602dce.jpg




imgrId51306a452e2833b17.jpg




imgrId52106a452e253a90a.jpg




imgrId52276a452e25bb605.jpg




imgrId52546a452e26775aa.jpg




imgrId52556a452e27aa8c8.jpg




imgrId53336a452e260dc4e.jpg




imgrId53956a452e27d4b2b.gif




imgrId54660119.jpg




imgrId54976a452e2703091.jpg




imgrId55596a452e278fa8f.jpg




imgrId56776a452e261b8f7.jpg




imgrId57366a452e28b327f.gif




imgrId57876a452e27cfbdb.jpg




imgrId58996a452e28cd42f.jpg




imgrId59216a452e2756d97.jpg




imgrId60636a452e27388e5.jpg




imgrId60956a452e27b5d77.jpg




imgrId61416a452e25acf20.gif




imgrId62016a452e26effbb.jpg




imgrId62866a452e2869e61.jpg




imgrId62926a452e26cd2ba.jpg




imgrId63026a452e26e91c6.jpg




imgrId63286a452e26a1a40.jpg




imgrId63826a452e277685d.jpg




imgrId64506a452e267cf3a.jpg




imgrId65846a452e27ef637.gif




imgrId65956a452e28928e6.jpg
'@E 1

s T T





imgrId66906a452e25eaa96.jpg




imgrId67426a452e28e8302.jpg
-:ﬁ___
i-=ﬂn—_
T

14




imgrId68026a452e28af018.jpg




imgrId68876a452e27622b3.jpg




imgrId69426a452e259264e.jpg




imgrId70236a452e28e103c.jpg




imgrId70376a452e2851fd3.png




imgrId71076a452e250e712.gif




imgrId72506a452e274eea0.jpg




imgrId72856a452e25079bd.jpg




imgrId73456a452e27a34f3.jpg




imgrId73496a452e26280e2.jpg




imgrId74286a452e28f40ff.gif




imgrId74516a452e252e1e0.jpg




imgrId75076a452e251e8cd.jpg




imgrId76276a452e278869d.jpg
L=
id




imgrId80586a452e28a7dc8.jpg




imgrId80606a452e2652fdc.jpg




imgrId80646a452e280d492.jpg




imgrId80896a452e28c6397.gif




imgrId80986a452e2907a18.jpg
A





imgrId82006a452e270d1b7.jpg




imgrId82266a452e2535e59.jpg




imgrId82346a452e2840f3d.png




imgrId82906a452e27bf372.jpg




imgrId84996a452e2669d4a.jpg




imgrId86396a452e2747745.jpg




imgrId86726a452e25b37dc.jpg




imgrId86766a452e25c0360.gif




imgrId90126a452e268493d.jpg




imgrId90196a452e256b913.jpg




imgrId90226a452e25a819b.jpg




imgrId90366a452e25488aa.jpg




imgrId90376a452e25d4bf6.jpg




imgrId91186a452e271249f.jpg




imgrId93416a452e2564adc.jpg




imgrId94196a452e279b9eb.jpg




imgrId94336a452e2767bf8.jpg




imgrId94436a452e2866258.jpg




imgrId94816a452e2541085.jpg




imgrId95366a452e2752e8b.jpg




imgrId95596a452e2828abd.jpg




imgrId96566a452e271fb49.jpg




imgrId96996a452e281c5ef.gif




imgrId97476a452e2614ebd.jpg




imgrId97556a452e28f0ba2.jpg




imgrId98006a452e27ad111.gif




imgrId98106a452e28d5598.jpg




imgrId99046a452e27c59a2.jpg




imgrId99316a452e262cc13.jpg




image1.png
™ rehlko




