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Information about optional components

Heater (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.1.1 Disassembly


1. Undo the screws A .
2. Remove the flange C .
3. Remove the heater E and the relevant gaskets F .
	[image: ]
Fig 11.1

	11.1.2 Assembly
 
[image: ]   Important
 
 
· Always replace gaskets F , with each assembly.

 
1. In sequence, fit the manifold G with the gasket F , the new heater E , the second gasket F , the flange C , the washers H , the screws A and the cable B .
2. Secure the flange C with the screws A (tightening torque at 22 Nm ).
	[image: ]
Fig 11.2


 



Idler gear (for 3rd / 4th PTO)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.2.1 Disassembly


1. Perform the operations of point 7 of Par. 7.4.1 .
2. Perform the operations from point 2 to 3 of  Par. 6.6.1 .
3. Perform the operations of point 3 of  Par. 7.8.1 .
4. Perform the operations of Par. 7.8.2 .
5. Loosen capscrews A and remove plate B1 .
6. Extract gear C .
7. Remove gudgeon D together with plate B2 .
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Fig 11.3
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Fig 11.4

	11.2.2 Assembly
 
[image: ]   Important
 
 
· Make sure that gudgeon D has no impurities inside.

 
1. On capscrew A , assemble:

    - plate B1
    - gudgeon D
    - gear C  
    - plate B2 .
	[image: ]
Fig 11.5



	1. Position gear unit C1 onto crankcase E , complying with reference J1 , J2 with gear F .
2. Secure unit C1 by means of capscrew A (tightening torque 25 Nm ).
NOTE: the reference J1 can have 2 different configurations for the gear C , Fig. 11.6b shows the correct position of the reference J1 for both configurations.
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Fig 11.6


[image: ]


[image: ]
Fig 11.6b




 



3rd PTO (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.3.1 Disassembly


1. Perform the operations of point 7 of  Par. 7.4.1 .
2. Perform the operations from point 2 to 3 of  Par. 6.6.1 .
3. Perform the operations of point 3 of Par. 7.8.1 .
4. Perform the operations of Par. 7.8.2 .
5. Extract gear A .
	[image: ]
Fig 11.7

	11.3.2 Assembly


1. Insert gear A into the seat of crankcase B , fitting the shaft of pump C in gear A .
	[image: ]
Fig 11.8


 



4th PTO (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.4.1 Disassembly


1. Perform the operations of point 7 of  Par. 7.4.1 .
2. Perform the operations from point 2 to 3 of  Par. 6.6.1 .
3. Perform the operations of point 3 of Par. 7.8.1 .
4. Perform the operations of Par. 7.8.2 .
5. Extract gear A .
	[image: ]
Fig 11.9

	11.4.2 Assembly


1. Insert gear A into the seat of crankcase B , fitting the shaft of pump C in gear A .
	[image: ]
Fig 11.10


 



Balancer device (replacement)
	[image: ]   Importante
 
 
· Before proceeding with operation, read Par. 3.3.2 .

	11.5.1 Disassembly


1. Perform the operations described in Par. 11.2.1 .
2. Extract shaft A1 e A2.
	[image: ]
Fig 11.11

	11.5.2 Assembly


1. Lubricate gudgeon C of shaft A1 and A2 with oil.
2. Insert shaft A1 into seat B1 of the crankcase, complying with reference D of gear E .
3. Insert shaft A2 into seat B2 of the crankcase.
4. Perform the operations described in Par. 11.2.2 .
NOTE: the shafts A1 and A2 are different and it is important not to invert the assembly position, the reference D is specific for the shaft A1 and is timed with the gear E , the reference J2 is specific for the shaft A2 and is timed with the idler gear F (see the Fig. 11.12b ).
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Fig 11.12


[image: ]     [image: ]
Fig 11.12b




 



ETB (replacement)
	1. Unscrew screws A and remove the ETB valve B with its gasket C . 
 
[image: ]   Important
 
 

 

· Always replace the gasket C  at each assembly.
	[image: ]
Fig. 11.13

	1. Fix the ETB valve B and its gasket C by means of screws A (tightening torque 10 Nm )
	[image: ]
Fig. 11.14


 



Air filter (cartridge replacement)
	1. Release the two hooks F and remove the cover A from the body D .
2. Remove the cartridges B and G .

 
 
[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
· The safety cartridge G (if present) must always be replaced if it is dirty or damaged.


1. Insert the new cartridge G inside the new cartridge B and both of them inside the filter body D .
2. Secure the cover A via the hooks F .
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Fig 11.59


 



Cooling circuit (replacement)
	[image: ]   Important
 
 
· Before proceeding with operation, read  Par. 3.3.2 .
· Before carrying out the operation, refer to the machine manual to disconnect the fuel waste line from the fuel radiator C2 .
	[image: ]

	11.8.1 Smontaggio vaschetta di espansione *


1 - Release the clamp A1, A2 .
2 - Disconnect hose B1, B2, B3 .
3 - Loosen capscrews C1 .
4 - Loosen capscrews C3 e rimuovere la vaschetta C4 . *
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	11.8.2 Radiator d isassembly



1 - Release the clamp A3, A5 .
2 - Disconnect hose B4 from radiator C .
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	4 - Release the clamp A2, A4, A5 .
5 - Disconnect hose B3, B5 from radiator C .
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[image: ]

	6 - Loosen all capscrews E1, E2, E3.
7 - Release nut F .
8 - Remove floodgates G1 and G2 .
9 - Loosen capscrews K .
10 - Disconnect radiator C from hoses H1 and H2 , being careful not to deform tubes J1 and J2 .




	[image: ]
[image: ]
[image: ]
[image: ]
[image: ]

	11.8.3 Fuel radiator replacement



1 - Loosen the screws E4 , extract the radiator C2 from the conveyor C1 .
2 - Insert the radiator C2 in the conveyor C1 .
3 - Fasten the radiator C2 with the screws E4 and washers E5 (tightening torque of 10 Nm ).
	[image: ]
[image: ]
[image: ]

	11.8.4 Fan disassembly


1 - Undo the screws P and remove the fan R .
	[image: ]

	  11.8.5 Fan assembly



1 - Assemble the fan R on the pulley U .
2 - Fasten the fan R by using the screws P (tightening torque at 10 Nm ).
	[image: ]





	11.8.6 Radiator assembly


1 - Insert the vibration damper V2 correctly on bracket S .

2 - Fit radiator C onto hose H1 , H2 being careful not to deform tube J1 , J2 .
3 - Centre radiator C onto vibration-dampening devices V .
4 - Secure radiator C onto vibration-dampening devices V by means of capscrews K (tightening torque at 25 Nm ).
5 - Fix the vibration damper V2 on the bracket S through the nut F (tightening torque of 25 Nm ).
6 - Secure hose H2 by means of clamp A5 .
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	7 - Position floodgate G1 onto radiator C .
8 - Secure all capscrews E1 , E3 , E2 .
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	9 - Secure hoses B3, B4, B5 by means of clamps A2 , A3, A4 .
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	11.8.7 Montaggio vaschetta di espansione *



1 - Fissare la vaschetta C4 sul radiatore C tramite le viti C3 (coppia di serraggio a 25 Nm ). *
2 - Fissare i manicotti B3, B1, B2 tramite le fascette A1 , A2 . *
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