|  |
| --- |
| **Flashing** |
| **Diagnostic tool manual** |



Sommario

[1. TITOLO 1 2](#_Toc495648770)

[1.1. Asdfsdfsdf 2](#_Toc495648771)

[1.2. Asdfsdfsdfggg 2](#_Toc495648772)


# Flashing

## Map download from the KOHLER server


|  |
| --- |
| Go to websiteo [**"http://iservice.lombardini.it"**](http://iservice.lombardini.it/)  and click on "KDI KOHLER DIESEL"  Read carefully "PRIVACY" box and click on  "I ACCEPT"  DIAGBOX_3.1_IT.jpg  Enter the "Username and Password", flag "I AM NOT A ROBOT" and clicking "Log-in".  DIAGBOX_3.3_EN.jpg  Click on "DIAGNOSIS AND FLASHING"  DIAGBOX_3.6_EN.jpg  Click on "FLASHING"  DIAGBOX_5.4_EN.jpg  Enter the Username and Password, then click on "Login"  DIAGBOX_5.5.jpg  Click on "Flashing ROM"  DIAGBOX_5.6.jpg  Click on "Obtain MAC address" (1) and then enter the "Serial number" (2). Click on "Search" (3) and then "Download" (4).  DIAGBOX_5.7.jpg  Z_Pericolo.jpg  **Warning**  If the "MAC address" is not detected automatically, perform the following operations:  Click on "START" > "All programs" > Accessories > Command prompt.  DIAGBOX_5.8_EN.jpg  Write: **ipconfig/all.**  DIAGBOX_5.9.jpg  Press enter.  DIAGBOX_5.10_EN.jpg  Per i PC portatili, nella scheda "LAN wireless Connessione rete wireless" è indicato il numero dell' "Indirizzo fisico"; per i PC fissi l'indirizzo fisico si trova nella scheda "Ethernet Ethernet".  Each computer has a different number.  Write down the physical address number (1) (separating the numbers with ":" and no longer with "-") in the "MAC address" field of the PC.  Enter the "Serial number" (2) and then click on "Search" (3).  DIAGBOX_5.11.jpg  When the search is complete, the name of the file will appear, identified by the engine K of the relevant map.  DIAGBOX_5.12_IT.jpg  Click on "Download" (4) and click on "Save" (5).  DIAGBOX_5.13_IT.jpg  The file will be saved automatically to the "Download" folder of the computer.  DIAGBOX_5.14_IT.jpg |


## Flashing

Press the "Check" push button to access the "Diagnosis" display screen.




Click on "UPDATE MAPS" and wait some seconds.







Turn on the panel and press "OK"




Click on "REP.ECU." (ECU reprogramming).



Click on "YES".



Wait some minutes.



Click on "OK".

