|  |
| --- |
| **Information regarding discharge of liquids** |
| **KDI 2504 TM Workshop manual (Rev. 07.6)** |



Sommario

[1. TITOLO 1 2](#_Toc495648770)

[1.1. Asdfsdfsdf 2](#_Toc495648771)

[1.2. Asdfsdfsdfggg 2](#_Toc495648772)

# Information regarding discharge of liquids

## Coolant

|  |  |
| --- | --- |
| Z_importante.jpg  **Important**  * Before proceeding with operation, read  [**Par. 3.3.2**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=437&parent=1527) .

**N** **OTE:** Component not necessarily supplied by **KOHLER** .The representation of the radiator is purely indicative.  Z_Avvertenza.jpg **Warning**  * Presence of steam pressurized coolant danger of burns.

 1. Undo the cap **A** carefully (circuit under pressure).
 | 5.1.jpg**Fig 5.1** |
| 1. Loosen cap **D** , remove gasket **E** , drain all coolant in radiator **G** into a suitable container and refer to  [**Par. 3.6**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=288&parent=1527) .
 | 5.2.jpg**Fig 5.2** |
| 1. Undo cap **F** to drain all liquid from the system contained in the engine crankcase ducts into an appropriate container and refer to [**Par. 3.6**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=288&parent=1527)

  | 5.3.jpg**Fig 5.3** |
| **NOTE** : Click by side to play the procedure. | <https://www.youtube.com/embed/QqQVCC4FAxA?rel=0> |

## Engine oil

|  |  |
| --- | --- |
| Z_Avvertenza.jpg **Important**  * This operation should be carried out with vacuum pump. The oil must be drained whilst the engine is hot, which requires particular care to prevent burns. Do not allow oil to come into contact with the skin because of the health hazards involved. It is recommended to use an oil intake pump via the oil dipstick hole **B.**
* Before proceeding with operation, read  [**Par. 3.3.2**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=437&parent=1527) .

**NOTE:** Perform this operation with warm engine, to get a better fluidity of the oil and get a full discharge of oil and impurities contained in it.1. Undo the oil filler cap **A** .
2. Remove the oil dipstick **B** .
3. Remove the oil drain plug **D** and the gasket **E** (the oil drain plug is on both sides of the oil sump).
4. Drain oil in an appropriate container.(For used oil disposal refer to the [**Par 3.6**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=288&parent=1527) ).
5. Perform the operations described in [**Par. 6.6.**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=660&parent=1527)
 | 5.4.jpg **Fig. 5.4** |
|   **NOTE** : Click by side to play the procedure. | <https://www.youtube.com/embed/Es7_GdKj1Wg?rel=0> |

