|  |
| --- |
| **Information about failures** |
| **KDI 1903 M Workshop manual (Rev. 09.6)** |



**Registration of modifications to the document**

Any modifications to this document must be registered by the drafting body, by completing the following table.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Released by** | **Code** | **Revision** | **Release Date** | **Revision date** | **Edited by** | **Endorsed** |
| Technical Documentation | ED005302-960 | 9.6 | 04/2013 | 03/2023 | M. SILVESTRONE | V. MANINI |

**Translated from the original manual in Italian language**

Data reported in this issue can be modified at any time by KOHLER.

Sommario

[1. TITOLO 1 2](#_Toc495648770)

[1.1. Asdfsdfsdf 2](#_Toc495648771)

[1.2. Asdfsdfsdfggg 2](#_Toc495648772)

# Information about failures

## Possible causes and trouble shooting

**IMMEDIATELY STOP THE ENGINE WHEN:**

1. Engine rpm increases and decreases suddenly without being able to control them;
2. A sudden and unusual noise is heard;
3. The colour of the exhaust fumes suddenly darkens or turns white;
4. The oil pressure warning light or a Warning Lamp turns on during operation;
5. The coolant temperature warning light turns on during operation.

**Tab. 14.1** contains the possible causes of some failures, which may occur during operation.

Always perform these simple checks before removing or replacing any part.

Z_Avvertenza.jpg **Warning**

* Search for a topic and the operations to carry out from the analytical index or chapter index found at the beginning of the manual.
* Do not carry out any checks or operations on the engine when it is running.

**Tab. 14.1**



