|  |
| --- |
| **Fluids filling information** |
| **KDI 3404 TCR-SCR Workshop Manual (Rev. 10.4)** |



**Registration of modifications to the document**

Any modifications to this document must be registered by the drafting body, by completing the following table.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Released by** | **Code** | **Revision** | **Release Date** | **Revision date** | **Edited by** | **Endorsed** |
|  | manoff |  |  |  |  |  |

**Translated from the original manual in Italian language**

Data reported in this issue can be modified at any time by KOHLER.

Sommario

[1. TITOLO 1 2](#_Toc495648770)

[1.1. Asdfsdfsdf 2](#_Toc495648771)

[1.2. Asdfsdfsdfggg 2](#_Toc495648772)

# Fluids filling information

## Engine oil

|  |
| --- |
| Z_Avvertenza.jpg **Warning**  * Before proceeding with operation, carefully read [**Par. 3.3.2**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=642&parent=1273) **.**

  |
| 1. Loosen the oil filler cap **A** .
2. Add the type and amount of oil recommended ( [**Tab. 2.2**](https://iservice.lombardini.it/jsp/Template2/manuale.jsp?id=101&parent=1273) ).
3. Remove the oil dipstick **B** and check that the level is up to but does not exceed the **MAX** .

  Z_importante.jpg **Important**  * Do not use the engine with the level of oil below **MIN** or above **MAX**
1. If the oil level is not at **MAX** , insert more oil until the **MAX** level is reached as indicated on the dipstick.
2. Re-tighten the cap **A** .
 | 10.1.jpg**Fig 10.1** |
| 10.2.jpg**Fig 10.2** |
| **NOTE** : Click by side to play the procedure. | <https://www.youtube.com/embed/HWCzK41Br1U?showinfo=0&rel=0> |

## Coolant

|  |
| --- |
| **NOTE** : Component not supplied by **KOHLER** .Refer to the technical documentation of the vehicle. |

