|  |
| --- |
| **Technical information** |
| **KSD 1403 owner manual (Rev. 00.1)** |



**Registration of modifications to the document**

Any modifications to this document must be registered by the drafting body, by completing the following table.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Released by** | **Code** | **Revision** | **Release Date** | **Revision date** | **Edited by** | **Endorsed** |
|  | KSD1403 |  |  |  |  |  |

**Translated from the original manual in Italian language**

Data reported in this issue can be modified at any time by KOHLER.

Sommario

[1. TITOLO 1 2](#_Toc495648770)

[1.1. Asdfsdfsdf 2](#_Toc495648771)

[1.2. Asdfsdfsdfggg 2](#_Toc495648772)

# Technical information

## General description of the engine

|  |
| --- |
| - 4-stroke, in-line cylinders Diesel engine; - Liquid-cooling system;    - 2 valves per cylinder;    - Indirect injection. |

## Engine specifications (base version)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **2.1**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | **TECHNICAL DATA** | | **UNIT OF MEASURE** | Cap_2_01.png | | | | **Engine type** | | | **KSD 1403 NA** | **KSD 1403 TC** | **KSD 1403 TCA** | | **Cylinders** | | n. | 3 | | | | **Bore** | | mm | 81 | | | | **Stroke** | | mm | 90 | | | | **Displacement** | | cm 3 | 1391 | | | | **MAX INCLINATION DURING OPERATION (even in combined)** | | α | 35° max | | | | α | 45° max 1 min. | | | | **OIL CAPACITY (MAX level.) including oil filter** | **Compact Sump** | lt. | 3.79 | | | | **Deep Sump** | 5.37 | | | | **DRY WEIGHT** | | kg | 124 | 128 | 127 | |

## Engine dimensions (mm)

|  |
| --- |
| **KSD 1403 NA** |
| Cap_2_03_04.png |
| **KSD 1403 TC** |
| Cap_2_05_06.png |
| **KSD 1403 TCA** |
| Cap_2_07_08.png |

**NOTE** : Dimensions vary according to engine configuration.

## Oil

Z_importante.jpg **Important**

* The engine may be damaged if operated with improper oil level.
* Do not exceed the **MAX** level because a sudden increase in engine rpm could be caused by its combustion.
* Use only the approved oil to ensure adequate protection, efficiency and service life of the engine.
* The use of lubricants other than recommended may shorten the engine life.
* Viscosity must be appropriate to the ambient temperature to which the engine is to be exposed.

Z_Pericolo.jpg **Danger**

* Prolonged skin contact with the exhausted engine oil can cause cancer of the skin.
* If contact with oil cannot be avoided, thoroughly wash your hands with soap and water as soon as possible.
* For the exhausted oil disposal, refer to the **Par.** **DISPOSAL and SCRAPPING** .

**2.4.1 SAE oil classification**

* In the SAE classification, oils are identified according to viscosity without considering any other qualitative characteristic.
* The code is composed of two numbers, which indicate, and must correspond to, the ambient temperature in which the engine operates, the first number refers to the viscosity when cold, for use during winter (" **W** "), while the second number is for viscosity at high temperatures.

**2.2**

|  |  |  |
| --- | --- | --- |
| **RECCMMENDED OIL** | | |
| **WITH SPECIFICATIONS** | **API** | CI-4 or better |
| **ACEA** | E7 or better |
| **VISCOSITY** | **SAE** | 0w-40 (-40°C ÷ +50°C)  10w-40 (-25°C ÷ +50°C) |

## Fuel

|  |  |
| --- | --- |
| Importante.png  **Important**   * Use of other types of fuel could damage the engine. Do not use dirty diesel fuel or mixtures of diesel fuel and water since this will cause serious engine faults. | Avvertenza.png  **Warning**   * Clean fuel prevents the fuel injectors from clogging. Immediately clean up any spillage during refuelling. * Never store diesel fuel in galvanized containers (i.e. coated with zinc). Diesel fuel and the galvanized coating react chemically to each other, producing flaking that quickly clogs filters or causes fuel pump and/or injector failure. * Any failure resulting from the use of fuel other than **Tab. 2.3, 2.4**  will not be covered by warranty. |
| **Cetane number of 40 minimum. Cetane number greater than 47 is preferred, especially for temperatures below –20 °C (–4 °F) or elevations above 1675 m (5500 ft.).**  **2.3**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | **Certification -->** | **Stage 5** | **Stage 3A**  **4** | **Tier III**  **IV** | **no certification** | **Remarks :** | | **Fuel Type -->** | (EN 590 - DIN 51628) | |  | (EN 590 - DIN 51628) | Do NOT USE vegetable oils as a biofuel not compliant with EN590 prescription. | |  |  | Grade 1-D S15 | | For ambient temperatures below 0°C (32°F) with no arctic fuel available (Grade 1-D S15, Grade 2-D S15, ASTM D 975) use the following additives to prevent possible engine damage with low engine load in cold weather:     * Power Service Diesel Fuel Supplement+Cetane Boost   Different additives are not allowed.  The use of approved additives has no impact on the engine maintenance schedule.  Do NOT USE vegetable oils as a biofuel not compliant with ASTM D975 Grade1 and Grade2 prescription. | | Grade 2-D S15 | |   **2.4**   |  |  | | --- | --- | | **FUEL ADDITIVES** | **Remarks** | | Fuel additives with biocide/algaecide functions only are allowed in case of storage of fuel in the tank for long periods (one year or more). | For suggested brands and types contact Kohler staff | | These additives must be diluted in the fuel following the product prescribed percentages when filling the tank. | | Additives with functions other than biocide / algaecide are not al-lowed. | | | |

## Coolant recommendation

|  |
| --- |
| A mixture of 50% demineralized water and 50% low silicate ethylene glycol based coolant liquid must be used. Use a Long Life or Extended Life Heavy Duty OAT coolant free of: silicates, phosphates, borates, nitrites and amines.    The following ethylene-glycol based engine coolant for all models within KSD engine family may be used:     * OAT (Organic Acid Technology) Low Silicate: **ASTM D-3306 D-6210** * HOAT (Hybrid Organic Acid Technology) Low Silicate: **ASTM D-3306 D-6210**   The above coolants in concentrated formulation must be mixed with distilled, deionized, or demineralized water. A pre-mixed formulation (40-60% or 50-50%) can be used directly when available.  Importante.png  **Important**   * Do not mix ethylene glycol and propylene glycol based coolants. Do not mix OAT and HOAT based coolant. OAT performance life can be drastically reduced if contaminated with nitrite-containing coolants. * Never use automotive-type coolants. These coolants do not contain the correct additives to protect heavy – duty diesel engines.   OAT coolants are maintenance free up to 5 years or 4000hrs of operation , provided that the cooling system is topped up using the same type of coolant. Do not mix different coolant types. Test the coolant condition annually with coolant test strips. HOAT are not all maintenance free and it is recommended to have SCA (Supplemental Coolant Additives) added at the first maintenance interval. |

## Battery recommendation

**Battery not supplied by Kohler**

**2.6**

|  |  |
| --- | --- |
| **RECOMMENDED BATTERIES** | |
| **STANDARD OPERATING CONDITIONS AMBIENT TEMPERATURE > -15°C** | |
| **BATTERY CAPACITY** | **BATTERY DISCHARGE CURRENT** |
| 70 Ah | SAE 650  EN 715 |

|  |  |
| --- | --- |
| **STANDARD OPERATING CONDITIONS AMBIENT TEMPERATURE < -15°C** | |
| **BATTERY CAPACITY** | **BATTERY DISCHARGE CURRENT** |
| 100 Ah | SAE 850  EN 935 |

